Product Name: NI-700, NI-900 Master Controllers (32M RAM) 
FG #: FG2105-03, FG2105-09

Current Firmware Version: 3.60.453
Release Date: 03/02/2011
Device ID: 0x012A (NI-700)
	   0x0138 (NI-900)

----------------------------------------------------------
Prerequisites
----------------------------------------------------------

Master build 300 or greater.  (see Programming Information)

Requires NI-Device firmware version of 1.30.8 or greater to fully utilize the enhancements. 
If NI-Device version 1.30.8 or later is loaded before this master firmware version, the 
integrated device (5001) will be unavailable until the master side firmware is upgraded. 

----------------------------------------------------------
Changes in this release
----------------------------------------------------------

- Added the ability to disable IP Device Discovery on the Network Settings Web page.
- Added Mio R3, AVX-400, and NXA-PDU-1508-8 Axlink types
- Removed erroneous "no help found" message from terminal "help security" request
- Fixed Telnet "set duet" command to support setting Duet memory greater than 99 for the new NI-X100/256
- Fixed an issue that could result in the integrated device (5001) reverting to a dynamic device number upon reboot.
- Fixed an issue that could result in master lockup when using ZeroConfig.
- Fixed an issue that could result in master lockup during MVP-9000i Ethernet Hot Swap.
- General stability improvements that prevent Master lockups under certain conditions.

----------------------------------------------------------
Known Issues 
----------------------------------------------------------
  
None

----------------------------------------------------------
Programming Information
----------------------------------------------------------

  If you currently have a firmware build less than 300, to upgrade to this
  version (or greater) the upgrade requires the following process:

  1. Download kit with build 300 (or greater) - Download of last component 
     will fail.
  2. Reboot master
  3. Wait until you have connectivity to the master or you have a blinking
     AXLink status LED. This may take a couple of minutes.
  4. Download kit with build 300 (or greater) again - Download should pass.
  5. Reboot master.
  6. Please wait. This will take a few minutes for file extraction and key SSH
     generation. When you have connectivity to the master or the AXLink LED is
     blinking the master is ready.

-------------------------------------------------------------------------------
