Product Name: NI-700, NI-900 Master Controllers (64M RAM)
FG #: FG2105-70, FG2105-90

Current Firmware Version: 4.1.419
Release Date: 12/17/15
Device ID: 0x012A (NI-700)
	   0x0138 (NI-900)

----------------------------------------------------------
Prerequisites
----------------------------------------------------------

None.

----------------------------------------------------------
Programming Information
----------------------------------------------------------

When upgrading to 4.x.x firmware from pre-4.x.x firmware for the
first time, the upgrade process and subsequent reboot can take
considerably longer than usual.  The NI-X00 upgrade can take 
more than 15 min.

Firmware should be loaded in the following order:

There is no change to the NI Device firmware (device 5001), but if upgrading this firmware:
1) Load the NI device firmware to the integrated device (normally 5001)
   For NI-700: SW2105_NI_700_Device_v1_30_8.kit
   For NI-900: SW2105_NI_900_Device_v1_30_8.kit
   The master must be rebooted following the installation of the
   integrated device firmware.

2) Load SW2105-90_Master_v4_1_369.KIT (or higher) to device 0 via NetLinx Studio
   and reboot the master.


----------------------------------------------------------
Changes in this release
----------------------------------------------------------
- Corrected problem with limited / no network communication following a power outage (xTrack RFI 24014).
- Corrected problem with socket communication timeout (xTrack RFI 24607)
- Corrected AMX Processors Vulnerable to SSLv3 POODLE by only supporting TLSv1.0 on HTTPS port (xTrack 25173)
- Corrected problem with no scroll bars on Touch Panel remote access via internet browser (xTrack 24842)
- Corrected LDAP checking to be case insensitive to match behavior of LDAP and NX masters
- Added support for IPv6 when displaying an NX master's IP address through DATA.SOURCEIP in a M2M connection
- Removed debugging account to prevent security vulnerability
- Fixed SSL certificate generation/request creation to accept non-default values

----------------------------------------------------------
Known Issues 
----------------------------------------------------------
- The DHCP lease information displayed via Telnet/Terminal 
  "get ip" does not reflect the actual time the lease was
  acquired nor when it will be renewed/released.

- If a Duet module, while loading during boot time, produces
  a Telnet error message: "java.lang.NoClassDefFoundError:
  org/xmlpull/v1/XmlPullParserFactory" you should update 
  the Duet Module to the latest version.

- Must use iWeather v1.1.6 or higher to operate correctly on
  4.x.x firmware.

- IE security does not allow G4WebControl to install by default and
  IE8 64-bit not supported.




