To use this upgrade package:  

This field upgrade package contains the following items.

Instructions.txt                text file
DGX_DVI_TX_v1.0.2.s19           Motorola S-Record file           PIC application code
ReadMe.txt                      text file
FWUpgradeTool_1.0.1.exe         executable file                  Software Application Installer code
                   

1. Read the readme.txt file and observe that all listed prerequisites for this upgrade are met.

2. Execute the FWUpgradeTool_1.0.1.exe file. This will install the Firmware Upgrade Application tool onto your system. Note that the Upgrade Utility has its own readme file. We recommend that you review the readme file for information about the installation and operation of the Upgrade Tool. If you already have this software installed on your system you can skip this step.

3. Step-by-step instructions for use of the Firmware Upgrade Tool to upgrade your DGX module are given in Appendix C of the “DGX Fiber TX & RX Modules Instruction Manual.” This can be obtained from:

http://www.amx.com//techdocs/AutoPatch/DGX-Fiber_TXRX_Modules.InstructionManual.pdf