DGX HD-15 RX firmware version v1.0.2, build date Nov 30 2010, 08:12:19


Note: 

The firmware is packaged in DGX_HD-15_RX_v1.0.2_Upgrade.zip file containing all archived pieces required to upgrade the device to the latest load.  Please read the Instructions.txt file for a detailed upgrading instructions.

As always, check JIRA database for a complete listing of bugs fixed in this build.  The release notes only highlight the major changes and those with the most visibility.

Prerequisites: Host software v1.0.0 or v1.0.1 must be installed and running before DGX_HD-15_RX_v1.0.2 can be installed. Host software is factory installable only. 

Checking following three items requires use of the USB port; for details on using the USB port, see the product’s Installation Manual. 

-- The PIC hardware driver image is compatible with host software version 1.0.1 and earlier. You can check the host software version installed on your DGX module by inspecting the splash screen info available at the USB port.

-- PIC hardware driver version DGX_HD-15_RX_1.0.2 is compatible with DGX HD-15 RX module hardware reporting a hardware id value of 02 or lower. The hardware id value may be observed from the USB splash screen in the [hardware id] field.


-- The software images provided in this upgrade package will generate the following splash screen. This is accessible from the USB port by executing the ~scr! command (see Product User 's manual for details of use of the USB port.)


[Accessory Module] AMX AutoPatch DGX ANALOG RX
    [host software] 1.0.1
    [hardware driver] 1.0.2
    [hardware id] 01
    [FPGA code] 0001001C
    [build date] Nov 30 2010, 08:12:19
[Temperature Sensors]
    [ambient] 33c
    [core] 50c

Changes in this release:

-- (JIRA HG-227 fixed) HGRX can get stuck in Pixel Dereplication mode when input video switches away from an ATX source 
-- (JIRA HG-228 fixed) HGRX - Pure PCLK video corruption
-- (JIRA HG-229 fixed) Implement Algorithm enhancement used in Hood for Bug DGXXLHW-171 VR/HR continuous scrolling



Known Issues:

-- (B3562) RS-232 data line active while switching upstream.Serial Data lost when Digital Audio change event happens.
-- (B3619) Can't communicate using some USB hubs. USB comm port does not get reestablished on a power cycle.
-- (B4018) ATX 1.0.2 Upstream video switch with audio in the system can cause double mute. 
-- (B4028) Rx: basic interlaced VTOT off +/-1 in bypass mod.


