Release Notes

NXR-ZGW ZigBee PRO Ethernet Gateway

FG#: FG5791-01 (original gateway)
     FG5791-11 (ZigBee Pro Gateway)

Current Firmware Version: 3.01.13
Release Date: 05/14/10

Device Id: x0134 


Prerequisites: v3.00.00.
-----------------------
1.  For the proper operation of all devices, it is recommended that all devices be
    brought up to the most current firmware version.

 
2.  Loading procedures for v3.01.13:

	When upgrading from any version less than v3.00.00:

	1.  Upgrade to v3.00.00 first (example:  v1.01.20 -> v3.00.00)
	2.  The upgrade from v3.00.00 to v3.01.11 will require two loads of the file
	    SW5791_01A_NXR_ZGW_v3_01_12.kit.  The first load will fail after the third
	    file is transferred with the NetLinx error message “Transfer Aborted -
	    Unsupported file type.”  After getting this error message, reboot the
	    gateway and verify that the NetLinx OnLine Tree shows v3.01.12 for the
	    version on the gateway.  Transfer file SW5791_01A_NXR_ZGW_v3_01_12.kit
	    to the gateway a second time with the “Reboot Device” box checked in NetLinx.
	    This time the entire kit file will transfer.  After the gateway reboots,
    	    it will download the firmware to the radio.  This will take approximately
	    two minutes.

	3.  Load SW5795_92_ZIGBEE_END_DEVICE_v3_01_05.kit -- a gateway reboot IS NOT
	    necessary after sending this file.

	4.  Load SW5791_07_ZIGBEE_REPEATER_v3_01_05.kit -- a gateway reboot IS NOT
	    necessary after sending this file.


	When upgrading from v3.00.00:

	1.  The upgrade from v3.00.00 to v3.01.12 will require two loads of the file
	    SW5791_01A_NXR_ZGW_v3_01_12.kit.  The first load will fail after the third
	    file is transferred with the NetLinx error message “Transfer Aborted -
	    Unsupported file type.”  After getting this error message, reboot the
	    gateway and verify that the NetLinx OnLine Tree shows v3.01.11 for the
	    version on the gateway.  Transfer file SW5791_01A_NXR_ZGW_v3_01_11.kit
	    to the gateway a second time with the “Reboot Device” box checked in NetLinx.
	    This time the entire kit file will transfer.  After the gateway reboots,
    	    it will download the firmware to the radio.  This will take approximately
	    two minutes.

	2.  Load SW5795_92_ZIGBEE_END_DEVICE_v3_01_05.kit -- a gateway reboot IS NOT
	    necessary after sending this file.

	3.  Load SW5791_07_ZIGBEE_REPEATER_v3_01_05.kit -- a gateway reboot IS NOT
	    necessary after sending this file.


	When upgrading from v3.01.07:

	1.  Transfer the file SW5791_01A_NXR_ZGW_v3_01_12.kit to the gateway via NetLinx
	    with the "Reboot Device" box checked in NetLinx.

    	    It is not necessary to reload SW5795_92_ZIGBEE_END_DEVICE_v3_01_05.kit or
	    SW5791_07_ZIGBEE_REPEATER_v3_01_05.kit since these files have not changed
	    in this release.
	2.  Recommission  all devices on the network.


Changes in this release
-----------------------

-- Fixed a bug where time update from the master could cause all devices to drop offline for a few seconds.
-- fixed a bug with using device number 0



Known Issues
------------
-- On systems that have one gateway and no repeaters, the remotes can become inoperable
   under extreme amounts of traffic (for example, 30 messages every two seconds to each
   of six remotes).  Rebooting these devices will bring them back online. 

-- The gateway does not currently support NDP mode for master connections.

-- In high traffic situations remotes can appear on the gateway commissioning page, even
   though they are commissioned.  This has no impact on the actual operation of the remotes.

-- In some cases, the R3 power source will show as “Unknown” on the gateway web pages when
   the R3 is in its cradle.  This issue does not impact the functionality of the remote
   or the gateway.



Programming Information
-----------------------
None.


