Product Name: MXA-MP
FG#: FG5968-20 MXA-MP, Modero X Accessory - Media Preview 

     
Current Firmware Version: 1.1.108
Release Date: 5/10/2013
Device IDs: N/A

Prerequisites: 
NONE


Changes in this release
-----------------------
-- Implemented bounds checking so that attempted video resolutions outside of the product's 
   capabilities return an error.  Resolutions at 60 fps are not supported.

Changes in release 1.1.103
--------------------------
-- Changed the Factory Defaults button semantics as follows:

	Reset Configuration Data to factory defaults:
	---------------------------------------------

	Press and Hold the 'Factory Defaults' button for about 5 seconds to request a change
	of the Configuration data back to factory defaults. The 'POWER' LED will blink 3 times
	to indicate that the system will now reset the configuration when the button is released.
	This will not affect the Firmware version. If you do not release the button after the '3 blinks'
	the system will proceed to keep counting towards the Firmware version factory default stage.
	The Configuration data default has now changed to 1280x720p@30 from ealier releases.

	Reset Firmware Version to factory default:
	-------------------------------------------

	Press and Hold the 'Factory Defaults' button for about 10 seconds to request a change to 
	the Firmware version back to the factory default. The 'POWER' LED will blink 3 times when
	it gets to the 'Configuration' stage. Keep HOLDING the button to continue the count to
	the 10 second 'Firmware' stage. When the 'POWER' LED blinks 7 times at a faster rate (about
	2x) than the 3-blink/(configuration) stage, it has then reached the 'Firmware' version
	factory default stage and will reset the firmware when the button is released.
	This will not affect the Configuration data.


-- Added additional video formats and resolutions to the '^SLT-1,videomode=<format>,<resolution>'
   send command. The following are now allowed:

	send_command 10001:1:0,"'^SLT-1,videomode=hdmi,640x480p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=hdmi,800x600p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=hdmi,1024x768p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=hdmi,1280x720p@30'"

	send_command 10001:1:0,"'^SLT-1,videomode=dvi,640x480p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=dvi,800x600p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=dvi,1024x768p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=dvi,1280x720p@30'"

	send_command 10001:1:0,"'^SLT-1,videomode=vga,640x480p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=svga,800x600p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=xga,1024x768p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=wxga,1280x768p@30'"

	send_command 10001:1:0,"'^SLT-1,videomode=component,720x480i@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=component,720x480p@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=component,720x576i@30'"
	send_command 10001:1:0,"'^SLT-1,videomode=component,720x576p@25'"

	send_command 10001:1:0,"'^SLT-1,videomode=svideo,ntsc'"
	send_command 10001:1:0,"'^SLT-1,videomode=svideo,pal-bghid'"
	send_command 10001:1:0,"'^SLT-1,videomode=svideo,pal-m'"

	send_command 10001:1:0,"'^SLT-1,videomode=composite,ntsc'"
	send_command 10001:1:0,"'^SLT-1,videomode=composite,pal-bghid'"
	send_command 10001:1:0,"'^SLT-1,videomode=composite,pal-m'"


Known Issues
------------
-- Video input format reports as PAL-BGHID on the ModeroX if no source is connected 
   and the configuration is set for COMPOSITE,NTSC. It corrects itself after the COMPOSITE
   cable is connected.

-- Due to the wide variety of video graphics cards on the market it is possible
   that some video chipsets may not work properly when connected directly to the
   MP(L), especially when using the VGA, SVGA, XGA, and WXGA formats. The chipsets 
   that have been tested (though others may also work) are:

	Intel(R) HD Graphics 3000
	AMD Radeon HD 6750M 
	NVIDIA GeForce 8200M G
