Product Name: N-Series N1x22A Video Encoder/Decoder
FG #: FGN1122A-SA (NMX-ENC-1122A)
      FGN1222A-SA (NMX-DEC-1222A)
      FGN1122A-CD (NMX-ENC-1122A-C)
      FGN1222A-CD (NMX-DEC-1222A-C)

Version: v1.15.45
Release Date: 01/21/2021

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- None

----------------------------------------------------------
2. Revision History
----------------------------------------------------------
Version 1/21/2021 (v1.15.45)
•	Fix analog audio stops after volume commands

Version 1/08/2021 (v1.15.44)
•	N1xxx updated number of slides per playlist to 8

Version 10/02/2020 (v1.15.43)
•	Fixes IR issues

Version 4/22/2020 (v1.15.41)
•	LLDP enables class 3 power for POE switches

Version 2/7/2020 (v1.15.40)
•   Add new command to create dhcp timing extended
    New command "setSettings:dhcpAgain:300", after
    300 seconds after the unit assigns itself an auto IP, the DHCP process
    would start again.  User can modify the 300 to value they need.

Version 12/13/2019 (v1.15.39)
•	Fix random dhcp failure after firmware update

Version 11/15/2019 (v1.15.38)
•	Fix commands not working randomly after a reboot

Version 10/31/2019 (v1.15.37)
•	Fix HDMI locking issue with certain laptops

Version 10/03/2019 (v1.15.34)
•	Fix various issues with VLAN tagging on Decoder

Version 10/03/2019 (v1.15.31)
•	Introduced VLAN tagging on Decoder

Version 07/18/2019 (v1.15.26)
•	Fixed version reporting incorrect on webpage.

Version 07/10/2019 (v1.15.25)
•	Remove VLAN Tagging for decoders for verification of encoders

Version 07/10/2019 (v1.15.24)
•	Fixed AES67 Packet Length with VLAN Tagging on N2000A Encoders

Version 07/10/2019 (v1.15.23)
•	Fixed AES67 Packet Length with VLAN Tagging on N1000A Encoders

Version 05/20/2019 (v1.15.21)
•	Added vlan tagging for video/audio on decoders

Version 04/10/2018 (v1.15.18)
•	Added a new optional IR method
•	Add commands for relative volume controls

Version 03/16/2018 (v1.15.17)
•	Netlinx bugfix - buffer RS-232 serial responses to minimize data events
•	Fix analog audio left/right bleed issue

Version 03/13/2018 (v1.15.16)
•	Improved IR output compatiblility 
•	Disable SSL ciphers in TLS1.1 and older
•	Improve detection of audio codec ESD event
•	Add option 'Resync HDMI on Live Play' for compatibility with some displays 

Version 02/12/2018 (v1.15.13):
•	Improve handling of serial data

Version 02/05/2018 (v1.15.12):
•	Correct issue with video artifacts
•	Improve audio codec ESD resilience
•	Updated web security to fix vulnerabilities

Version 01/05/2018 (v1.15.10):
•	Correct AES67 audio compatibility with QSC Core
•	NetLinx bugfixes

Version 11/27/2017 (v1.15.9):
•	Add support for Samsung Touchpanel
•	NetLinx bugfixes

Version 11/27/2017 (v1.15.8):
•	Correct playback of multichannel AES67 audio

Version 9/8/2017 (v1.15.7):
•	Corrected an issue with 1080i resolution

Version 9/8/2017 (v1.15.6):
 •	Fix potential issue where Hostplay can fail.

Version 8/31/2017 (v1.15.5)
•	Improved camera standby support
•	Improved detection of DVI vs. HDMI audio on certain sources
•	AES67 defaults to port 5004 on factory restore

Version 8/29/2017 (v1.15.4)
•	Added Stream Loss Action on web page and select None, HDMI Disable, or Standby mode
•	Audio codec recovers from ESD faster
•	AES67 limited to 239.x.x.x addresses

Version 8/2/2017 (v1.15.2)
•	Netlinx 0.0.32: Defaults to RXON to automatically handle string responses
•	Added additional HID touchscreens support
•	Interleaved audio streams output correctly when in MPC mode

Version 7/19/2017 (v1.15.1)
•	Improved handling of video sources in standby

Version 7/17/2017 (v1.15.0)
•	Added 'Display Hostplay on No Input' feature that turns off encoder transmit when no input detected
•	Added 'Disable HDCP Adveristing' feature that no longer provides HDCP negotiation on encoder input

Version 7/13/2017 (v1.14.15)
•	IR compatibility mode added for support of Foxtel devices
•	Host play for Non Supported Mode no longer forces a restart every 30 seconds
•	Netlinx 0.0.30: Bug fix
•	Added additional touchscreen support
Known bug(s): 1080i is currently encoding incorrectly.  Do not use this intermediate update on 1080i based installs.

Version 6/26/2017 (v1.14.14)
•	Improved ability for audio codec to recovery from ESD/shock

Version 6/14/2017 (v1.14.13)
•	Microphone bias added and default bias is now OFF

Version 4/03/2017 (v1.14.11b)
•	Correct time synchronization handling 
Version 4/03/2017 (v1.14.11)
•	Netlinx - Correct display of Svsi devices in Netlinx master webpage
•	Netlinx - Correct handling of 1024 byte buffered RS-232 Rx data
•	Netlinx- add VIDOUT_ON-[ON/OFF], modify VIOUT_MUTE to send/disable avmute
•	Netlinx- correct truncation of getStatus API response.
•	Increase KVM report size for Sharp touchpanel


----------------------------------------------------------
3. Known Issues
----------------------------------------------------------
