Release Notes

Product: PR01-RX
Description: Precis HDBaseT Receiver and Scaler
FG#: FG1020-050

File Name: SW1020-050_PR01-RX_v3_9
Firmware Version: 3.9
Release Date: 2020-12-16

!! Please read Programming Information for successful upgrade steps!!

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Known Issues
5. Programming Information
6. Notable Points


----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- NetLinx Studio v4.3.1519 (or later)

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
- Added ability to load and display a logo when no signal is present on a routed input
 -- Upload a single png logo file via WebUI
    -- Max image size 1280x720 & 60kB
 -- Control by WebUI or by NetLinx code
    -- VIDOUT_BLANK-<BLACK/LOGO>
 -- Choose fixed or moving logo option
    -- VIDOUT_LOGO-<FIX IN CENTER, DRAG TOP LEFT, etc>
- Added WebUI and NetLinx support for HDCP OUT setting 
 -- VIDOUT_HDMI_HDCP-<HDCP_FOLLOW, HDCP_2_2, HDCP_1_4, HDCP_OFF>
- Added WebUI volume control for HDMI output
- Updated WebUI and added certificate uploading function

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------
- Resolved issue of bootloader not closing serial port interrupt
  which caused receiving data interrupt on boot
- Corrected audio mute issue on HDMI disconnect
- Fixed HDMI OUT so it would persist HDCP setting over power cycle
- Modified HDMI OUT HDCP setting to default to FOLLOW after factory reset 
- Fixed SSL certificate errors
- Fixed USB audio distortion over HDBT link
- Fixed issue causing continual "Custom Event Type 1009" notifications


----------------------------------------------------------
4. Known Issues
----------------------------------------------------------
- None

----------------------------------------------------------
5. Programming Information
----------------------------------------------------------
- These devices can be updated using a VNM (Virtual NetLinx Controller)
  but the update will go much faster if you can connect to a physical
  NetLinx controller.  VNM update could take up to 2 hours but
  using a physical controller should take less than an hour.

- The update takes place in 3 stages.  The first part of the update
  happens during the Firmware Transfer in NetLinx Studio.  Once that
  transfer has completed the device will then continue the update and 
  show its progress in the Update Status page of the devices webgui.
  This must be selected prior to update and then it can be monitored.
  Once that update shows as completed the unit will then display the
  last stage of the update on a display connected to the HDMI output.
  The device will reboot when it has completed the full update.

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
- These units have a web interface that is accessible by entering
  the IP of the device into a web browser.  This may indicate there
  is a certificate error, but you can select the Advanced option at 
  the bottom and proceed to the page.  A new certificate can be loaded
  via the web interface.
