Release Notes

DXLink Fiber Receiver Firmware (Enova DGX 100 Series
Compatible)

!!This firmware version requires Enova DGX 100 Series
compatibility on connected Enova DGX systems!!

!!!Please reference the Enova DGX Board and Endpoint
Compatibility Instructions on the AMX.com product
page for more information!!!

FG#:
  FG1010-560 (DXF-RX-SMD, DXLink HDMI Single Mode Fiber Receiver, Duplex)
  FG1010-561 (DXF-RX-SMS, DXLink HDMI Single Mode Fiber Receiver, Simplex)
  FG1010-562 (DXF-RX-MMD, DXLink HDMI Multimode Fiber Receiver, Duplex)
  FG1010-563 (DXF-RX-MMS, DXLink HDMI Multimode Fiber Receiver, Simplex)


Release Date: 2017-07-14
Current Released Firmware: v1.4.19
SW1010_56x_AVB_KIT_DXLF_RX_v1_4_19.kit

----------------------------------------------------------
Table of Contents
----------------------------------------------------------

1. Prerequisites
2. Features added in this release
3. Fixes in this release
4. Notable points
5. Programming information

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- DXF-TX-xxD v1.4.9 (or later) to support standalone
  configuration.

- Enova DGX DXLink Fiber I/O boards must be upgraded to the
  latest firmware versions (as provided in the DGX kit file
  listed below).

- Enova DGX 100 Series enclosures need Enova DGX
  800/1600/3200/6400 FW v3.0.20 (or later) and Controller FW:

    - SW1060 v1.4.72 (or later)

- Enova DGX 8/16/32/64 enclosures need Enova DGX 8/16/32/64
  FW v2.2.8 (or later) and Controller FW:

    - SW1056 v4_2_395.KIT or later (NI-Series)
      Shows in Online Tree as "NI Controller"

    - SW2106_NX-X200 v1_3_110.kit or later (NX-Series)
      Shows in Online Tree as "DGX Controller"

- NetLinx Studio v4.3.1519 or later

----------------------------------------------------------
2. Features added in this release 
----------------------------------------------------------

- Added access to the superuser debug console via the RX's
  USB Program on the front panel (baud 115200) 
  Warning:  Use this port carefully as it is possible to 
  delete firmware or other necessary parameters

----------------------------------------------------------
3. Fixes in this release 
----------------------------------------------------------
- Fixed issue causing a factory reset during upgrade to v1.4.18

(Fixed in previous release 1.4.18)
- Fixed offline issue caused by Nessus network scans 
- Fixed issue where RX could bounce offline randomly
- Changed the default setting of VIDOUT_SLEEP to ENABLE
- Changed the default setting of VIDOUT_BLANK to BLUE
- Fixed a flash that could occur when source changed from 
  HDCP to non-HDCP (or on a disconnect of the route)

----------------------------------------------------------
4. Notable points
----------------------------------------------------------
-  IMPORTANT: Scaler settings upgrade warning
   If upgrading to DGX firmware v3.x.x from v3.0.10,
   and if DXLink RX are configured with non-default
   scaler settings (scaling mode, aspect ratio and
   manual resolution), the "PERSISTAV" ICSP command
   must first be sent to those RX's before performing
   the firmware upgrade of either the DGX or the RX's
   in order to preserve their modified settings.

- On duplex devices, if DIP switch 4 is set ON, the device
  will be put into unidirectional mode.  This will make the
  duplex device act similarly to a simplex device.
  Ethernet and control over the fiber link will be disabled.
  See the instruction manual for details.

- Please read the documentation in regard to the DIP
  switches located on the bottom of the Tx/Rx modules
  before attempting to connect to the network.

- After a FACTORYAV (ICSP) or RESET FACTORY (telnet)
  command, a reboot of the endpoint is required.

- The RX module uses these solid color screen indications:

  ORANGE
    Indicates an HDCP authentication failure with
    the connected HDMI sink (monitor or other device).

- If using a hostname in the USB_HID_ROUTE command,
  the hostname length is limited to 50 characters.

----------------------------------------------------------
5. Programming information
----------------------------------------------------------

- DXLink Fiber Receiver Firmware (Enova DGX 100 Series
  Compatible)

- !!This firmware version requires Enova DGX 100 Series
  compatibility on connected Enova DGX systems!!

- !!!Please reference the Enova DGX Board and Endpoint
  Compatibility Instructions on the AMX.com product
  page for more information!!!
