Product Name: N-Series N2300 Video Encoder/Decoder
FG #: FGN2312-SA
      FGN2322-SA

Version: 01.01.26
Release Date: 9/16/2021

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- None

----------------------------------------------------------
2. Revision History
----------------------------------------------------------
Version 01.01.26
• HDR support added
• feature support for input audio for hostplay/localplay
• fixed netlinx native command usage
• added support for secure netlinx connection
• fixed N2300 encoder reporting resolution to SVSI software 
• updated TLS to TLS  1.2 only

Version 01.01.25
• Fix dscp values used on webpage
• New values allowed from webpage are listed below:
{0, 8, 10, 12, 14, 16, 18, 20, 22, 24, 26, 28, 30, 32, 34, 36, 38, 40, 46, 48, 56}

Version 01.01.24
• Remove support for TLS 1.0 and 1.1 (use force https on webpage to ensure only TLSv1.2 utilized)

Version 01.01.23
• Optimize time delay in KVM IP switching

Version 01.01.21
• Fix webpage security issue with POST

Version 01.01.20
• Make more DHCP attempts during unit boot up
• Add new command to create dhcp timing extended
  New command "setSettings:dhcpAgain:300", after 300 seconds after
  the unit assigns itself an auto IP, the DHCP process
  would start again. User can modify the 300 to value they need.
  lower limit is 60 seconds, to allow linkLocal to work properly
  To disable the setting, "setSettings:dhcpAgain:0"

Version 01.01.18
• Improve the "Unsolicited Status" feature

Version 01.01.17
• Enable scaler of decoder after factory restoration

Version 01.01.16
• Fix issue where decoder reboots when unexpected
• Analog audio chip driver improvements

Version 01.01.15
• Improve VGA/HDMI startup time
• Implement option to give VGA or HDMI input priority
• Add Identify button to web page that displays IP address on decoder

Version 01.01.14
• Improve KVM connection recovery on reboot.
• Change audio stream ttl to default to 64
• Implement KVM retry
• Make analog audio startup delay optional
• Add optional encoder reboot on audio input failure

Version 01.01.05
•  Fix issue with uploading odd host/local play images
•  Fix issue with debug log startup
•  Fix issue with KVM reconnecting on encoder or decoder restart
•  Improved button feedback on webpages
•  Treat stream 0 as a stream instead of as a local play command
•  Add HDCP connection status to the decoder 
•  Resolved audio stream compatibilty issues with other N-Series units
•  Fixed audio multicast address calculation
•  Add option to blank video during switch
•  Don't issue NAct plug events on bootup
•  Improved audio networking to avoid audio pops when video rate goes up
•  Delay audio startup to avoid audio artifact after stream switch
•  Add option to disable video genlock which causes some monitors to stutter the audio
•  Improve decoder robustness 

Version 00.04.22
•  Fix audio multicast address for non-interleaved mode

Version 00.04.21
•  Fix 32K and 44.1K audio issue that occurred with selected monitors
•  Default output to RGB to avoid the green screen
•  Default KVM to on to match spec

Version 00.04.20
•  Fix audio pop on decoder analog audio output
•  Add 1920x1200 to EDID (requires reloading default EDID).
•  Add latest netlinx support and add netlinx version to the webpage

Version 00.04.15
•  Fix audio stutter issue
•  Add control for video genlock
•  Fix issue with audio channel count change crashing encoder.
•  Fix issue with log overflowing on debug start
•  Add support for DNS

Version 00.04.11
•  Provide sync override feature for monitors that are sensitive to clock changes.
•  Fixed decoder issue caused by selecting stream 0.  Now is the same as localPlay.
•  Fix IR upload for N2300 devices

Version 00.04.08
•  Fix loss of I-Frame requests on encoder stream restart

Version 00.04.04  
•  Add commands for output volume up/down 
•  Support secure ports only mode
•  Clean up xml status file
•  Improve encoder HDCP robustness
•  Add line input volume control  
•  Fix decoder reboot on stream switch
•  Suport RGB 4K resolution mode
•  Block unknown multicast streams from the swtich
•  Support Harman serial number format
•  Fix network lockup when switching into DHCP mode
•  Improved Netlinx support
•  Improved decoder stability

----------------------------------------------------------
3. Known Issues
----------------------------------------------------------

• On soft reboot, some devices lose KVM connectivity and require a hard decoder reboot
• If DHCP is first enabled on a network without a DHCP server, the unit reboots and the 
  setting is lost.  If the unit is running DHCP but is rebooted on a network without a 
  DHCP server, it falls back to autoip correctly.
