Release Notes

Product: PR-0808
Description: Precis 8x8 4K60 HDMI Switcher
FG#: AMX-PR-0808

File Name: SW_AMX-PR-0808_V1_55
Firmware Version: 1.55
Release Date: 2021-12-01

!! Please read Programming Information for successful upgrade steps!!

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Known Issues
5. Programming Information
6. Notable Points


----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- None

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
- Added IPv6 API commands. 
- Made OSD position adjustable. 
- Took out the System/Network/Security Commands on serial port. 
- Added command feedback for "incorrect command" and "incorrect parameter"
- Added 60 seconds time out for indirect control APIs.

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------
- Fixed the issue: SSH cannot get corresponding message after telnet turns from off to on.
- Fixed the issue: the unit cannot get the domain name and DNS information from DHCP server.
- Fixed the command feedback typos. 
- Fixed the Set commands issue - If no input data, it will keep current parameter.
- Adjusted the OSD postion to avoid OSD being cut off in overscan screen. 
- Changed the EDID libaray to avoid unexpected output resolution. 

----------------------------------------------------------
4. Known Issues
----------------------------------------------------------
- There may be wrong video resolution information on web UI for some uncommon video resolution. 

----------------------------------------------------------
5. Programming Information
----------------------------------------------------------
Firmware Upgrade through WebGUI
The system will be non-operational during the upgrade procedure below.
1. In the Switcher Configuration menu, enter the “System” page and then click “Browse” in the Firmware Update
Column to open the file selection window.
2. Select the appropriate file from the target directory.
3. Click “Update” to start firmware upgrading. The progress displays on both web UI and LCD display.
4. The unit finishes upgrading and auto reboots to active.

Firmware Upgrade through USB
The system will be non-operational during the upgrade procedure below.
1. Copy firmware file to folder in USB original disk
2. Insert USB Disk to USB Type A program port
3. Navigate the front panel LCD display to start firmware upgrade - SYSTEM SETUP > FIRMWARE UPDATE > YES.
   The progress displays on LCD display.
4. The unit finishes upgrading and auto reboots to active.

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
- None
