Release Notes

Products: JPK-1300-UA, JPK-1300-EK
Description: AMX Jetpack Kit includes Receiver, Wallplate Transmitter, and Keypad
FG#: AMX-VTK0001 (US and Asia)
     AMX-VTK0001EK (Europe and UK)

File Name: SW_AMX-JPK-1300_v1.04.01.bin
Release Date: 12/19/2022
Firmware Version: V1.04.01

   - Receiver：     V1.04.01
   - Wallplate TX: V1.01.11
   - Keypad：       V1.01.08
   - Web：          V1.00.23


1. Prerequisites 
2. Features added in this release
3. Fixes in this release:  
4. Known Issues  
5. Programming Information  
6. Notable Points  

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- Requires v1.03.10 or later to update

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
- None

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------
MCU
 - Optimize time zone setting related operations

Webgui
 - Fixed the time format
 - Disable Time Zone function and optimize logic when Set Time
   Automatically is set to OFF
 - Corrected an issue where saving the Schedule did not notify 
   user if the save was successful

FW
 - Fixed issue where the product would not get the IPv6 address 
   assigned by IPv6 server
 - Fixed audio/video issue when switching output mode between 
   "sharing the screen" and "Samsung DEX" using Type-C channel
 
API
 - Fixed "set dns" command
 - Corrected the IPV6 Mask Prefix (aka. Subnet Prefix Length) received 
   from the API command "get ipv6" to properly match the Webgui value 


----------------------------------------------------------
4. Known Issues
----------------------------------------------------------

----------------------------------------------------------

5. Programming Information
----------------------------------------------------------
- IMPORTANTE:  After upgrading the firmware, you must perform a factory reset, otherwise certain
  parameters are not initialized and the system as a whole may be in an abnormal state

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
 - USB2.0 SPDIF Audio requires 8s to be detected by USB-C Source when using USB2.0 Type-C to Type-C cable 