Release Notes

Products: JPK-1300-UA, JPK-1300-EK
Description: AMX Jetpack Kit includes Receiver, Wallplate Transmitter, and Keypad
FG#: AMX-VTK0001 (US and Asia)
     AMX-VTK0001EK (Europe and UK)

File Name: SW_AMX-JPK-1300_v1.04.03.bin
Release Date: 3/23/2023
Firmware Version: V1.04.03

   - Receiver：     V1.04.03
   - Wallplate TX: V1.01.11
   - Keypad：       V1.01.08
   - Web：          V1.00.25


1. Prerequisites 
2. Features added in this release
3. Fixes in this release:  
4. Known Issues  
5. Programming Information  
6. Notable Points  

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- Requires v1.03.10 or later to update

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
- None

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------

- Optimized Web Reboot feature so it will restart in the login interface automatically
- Resolved Save/Load config problem causing serial port commands to not be exported/imported properly in ASCII

Fixes in previous v1.04.02
Webgui
 - Clarify the private key supported format (both .key and .pem) for HTTPS certificate on the Webgui

FW
 - Fix feedback issue on Telnet/SSH when pressing either the “SOURCE” button on the Wall-plate TX 
   or pressing “HDMI 1”, “HDMI 2” and “USB-C” button on the keypad

Fixes in previous V1.04.01
MCU
 - Optimize time zone setting related operations

Webgui
 - Fixed the time format
 - Disable Time Zone function and optimize logic when Set Time
   Automatically is set to OFF
 - Corrected an issue where saving the Schedule did not notify 
   user if the save was successful

FW
 - Fixed issue where the product would not get the IPv6 address 
   assigned by IPv6 server
 - Fixed audio/video issue when switching output mode between 
   "sharing the screen" and "Samsung DEX" using Type-C channel
 
API
 - Fixed "set dns" command
 - Corrected the IPV6 Mask Prefix (aka. Subnet Prefix Length) received 
   from the API command "get ipv6" to properly match the Webgui value 


----------------------------------------------------------
4. Known Issues
----------------------------------------------------------

----------------------------------------------------------

5. Programming Information
----------------------------------------------------------
- IMPORTANTE:  After upgrading the firmware, it is best to perform a factory reset, to make sure any new or updated 
  parameters will get properly initialized

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
 - USB2.0 SPDIF Audio requires 8 sec to be detected by USB-C Source when using USB2.0 Type-C to Type-C cable
 - Below is a summary to get Video and full functionality of Jetpack USB-C (DisplayPort, KVM and SPDIF Audio over USB2.0)
 -- For USB Type-C Video: The cable and source must support "DP Alt Mode" 
 -- For USB-C Cable: Jetpack supports a maximum AV date rate up to 10Gbps (4K60:420 or 4K30/444), so the data transport 
    rate of the cable needs to support up to 10Gbps.  
 --- Based on DP Alt Mode for USB-C standard, USB-C Cable need compliant to:
 --- USB3.1 Gen1 (Equal to USB3.0) – 5Gbps (Lowest requirement to get full-feature of Jetpack USB-C connection)
 --- USB3.1 Gen2  –  10Gbps (Recommend requirement to get full-feature of Jetpack USB-C connection)
 --- Or higher version 