Release Notes

Product: PR-WP-412
Description: Precis 4x1+1 4K60 HDMI Windowing Processor
FG#: AMX-PR-WP-412

File Name: SW_AMX_PR-WP-412_v2_17.bin
Firmware Version: 2.17
Release Date: 2023-08-17

!! Please read Programming Information for successful upgrade steps!!

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Known Issues
5. Programming Information
6. Notable Points


----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- None

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------

- Added unsolicited feedback for valid vidin signal status for connect/disconnect activity

Features in Previous v2.16
- Added LDAPS & 802.1x functions.

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------

Fixes in Previous v2.16
- Fixed firmware Upgrade Web UI issue.
- Fixed can't SSH to WP after upgrade to V2.1x/2.0x firmware issue.
- Fixed poor image quality issue (color and vertical lines) 
  on windows 3 and 4 when switching windowing modes
- Fixed CEC control unavailable issue.
- Fixed LDAP/S feature fail issue.
- Fixed WebGUI [IEEE 802.1x Authentication] check box issue.
- Revised username & password from admin:admin to administrator:password
- Fixed Config saving issue->need to remove "Certificate Directory" in case that upload would fail.
- Fixed command typos.
- Removed certain unsupported formats from the EDID
- Unsupported Detailed Timing will be replaced with 1080p60
- Fixed Certificate with password reported "Update wrong password" issue.
- Fixed Telnet/SSH few setting commands feedback "incorrect parameter" issue.
- Fixed LDAP error that username can't use space.
- Fixed User Query Attr default would be "uid" issue.
- Fixed LDAP username character numbers issue.
- Fixed Web GUI login timeout issue
- Fixed Web GUI LDAP setting issue that revision would not be saved.
- Revised SSH account, password default to admin:admin.
- Revised web description.
- Fixed CEC manual power on/off function.

Fixes in Previous v1.67
- Fixed the issue where some settings are not saved in 
  configuration JSON file. 
- Fixed the issue where video sometimes color space error,
  video flashing or partial picture disappear. 
- Optimized the display native resolution detection. 
- Fixed the issue there is one additional video drop after
  video source changed. 


----------------------------------------------------------
4. Known Issues
----------------------------------------------------------
-None
----------------------------------------------------------
5. Programming Information
----------------------------------------------------------
Firmware Upgrade through WebGUI
The system will be non-operational during the upgrade procedure below.
1. In the Switcher Configuration menu, enter the “System” page and then click “Browse” in the Firmware Update
Column to open the file selection window.
2. Select the appropriate KIT file from the target directory.
3. Click “Update” to start firmware upgrading. The “Power” LED turns RED and keeps flashing.
4. Once the "Power" LED turns GREEN and stops flashing, the unit finishes upgrading and auto reboots to active.

Firmware Upgrade through USB
The system will be non-operational during the upgrade procedure below.
1. Copy firmware file to folder in USB original disk
2. Insert USB Disk to USB Type A program port
3. Press "reset" button on the rear panel 5 times in a row, and the unit starts upgrading when the “Power” LED turns RED
and keeps flashing.
4. Once the "Power" LED turns GREEN and stops flashing, the unit finishes upgrading and auto reboots to active.

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
- None
