Release Notes

Product: DXFP-TX-4K60
Description: DXLink 4K60 HDMI Fiber Transmitter Module

FG#: FG1010-365-01 
     FG1010-365-02 (TAA)

File Name: SW1010-365-0X_DXFP-TX-4K60_v1_8_5
Release Date: 3/22/2024
Firmware Version: v1.8.5

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Known Issues
5. Programming Information
6. Notable Points

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

 - Directly connected DXFP-RX-4K60 v1.8.4 (or later)
 - Enova DGX 800/1600/3200/6400 Switcher FW v3.8.25 (or later)
 - Enova DVX-2265-4K/DVX-3266-4K Switcher FW v1.9.4 (or later)
 - Enova DGX 100 Series & DVX 4K Series Controller FW v1.6.200 or v1.8.97 (or later)
 - NetLinx Studio v4.3.1519 (or later)

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
 - None
 
Added in previous release 1.8.4
 - Added telnet watchdogs to automatically recover endpoint MCU and MasterApp.  
   Syntax Notes: The command, by itself, queries the current setting. Using on/off after 
   the command will enable/disable the watchdog
	wdlog           Queries the count for each Recovery Mechanism (reset factory to clear) 
	wdmasterapp     Queries/enables/disables the masterapp Recovery Mechanism (default is on)
	wdmcu           Queries/enables/disables the MCU Recovery Mechanism (default is on)  
   
Added in previous release 1.8.3
 - Replaced MCU due to EOL parts.  FW updated to support new MCU processor

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------
 - Fixed test mode needed for manufacturing test
 
Fixed in previous release 1.8.4
 - Fixed a boot-up race condition causing endpoints to randomly be offline after a reboot
 - Fixed an RS232 issues with EVEN/ODD parity
 - Fixed a memory leak when using RS232 causing the endpoint to lockup over time requiring
   reboot to recover

Fixed in previous release 1.8.3
 - Fixed issue in TX/RX that caused RS232 strings to be passed out of order
  
 Fixed in previous release v1.8.0
 - Fixed Set Connection to Controller to support changing ICSP Port Number and URL hostname
 - Fixed async notifications for VIDIN_STATUS
 - Fixed Standalone webgui issue to allow changing Static IP and default Gateway together
 - Corrected issue causing IR File to be erased on upgrade (IR file should remain on subsequent upgrades) 
 - TX/ RX to change Eth0 default fallback to prevent conflict with DGX IO card IP scheme
 

----------------------------------------------------------
4. Known Issues
----------------------------------------------------------
 - None

----------------------------------------------------------
5. Programming Information
----------------------------------------------------------
 - These devices can be updated using a VNM (Virtual NetLinx Controller)
   but the update will go much faster if you can connect to a physical
   NetLinx controller. VNM update could take up to 2 hours but
   using a physical controller should take less than an hour.

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
 - PLEASE READ the Quick Start Guide in regard to the DIP switches located 
   on the DXLink 4K60 endpoint before attempting to connect to the network.

 - These units have a web interface that is accessible by entering
   the URL of the device into a web browser. This may indicate there
   is a certificate error, but you can select the Advanced option at
   the bottom and proceed to the page. A new certificate can be loaded
   via the web interface.

 - This web interface is only available when connected to a DXLink 4K60 Receiver.
   It is disabled when connected to other endpoint devices or a switcher.

 - This device has a default static IP: 192.168.1.2 when it isn't assigned a dynamic IP
   by DHCP server or auto-setup process.
