Product Name: CE-IRS4, CE-REL8, CE-COM2, CE-IO4

SKU #: AMX-CEB001, AMX-CEB002, AMX-CEB003, AMX-CEB004

Current Firmware Version: 1.2.7
Release Date: Aug 13, 2024

----------------------------------------------------------
Prerequisites
----------------------------------------------------------
None.

----------------------------------------------------------
Programming Information
----------------------------------------------------------
None.

----------------------------------------------------------
Changes in this release
----------------------------------------------------------
Version 1.2.7
- Fixed issue: Getfile Forwarding Header Missing from Block Message in HControl

Version 1.2.6
- Add support for some special characters in IR file
- Add support for some special characters in Open API commands sent from COM2 and IRS4
- Fixed issue: IRS4 does not send the pattern when function code “repeat end index” mismatch in IR file
- Fixed issue: clearAndSendNamedIr/onNamedIr/bufferedSendNamedIr command template of IRS4 are different from Muse

Version 1.2.5
- Fixed issue: some printable ASCII characters are ignored when sending strings with Open API from COM2 or IRS4
- Fixed issue: COM2 crashes when sending strings which are more than 50 ASCII characters with Open API

Version 1.2.4
- Improve stability when strings are sent from COM2

Version 1.2.3
- Add support for WolfSSL FIPS 140-3
- Add support for Open Control Protocol
- Update "locate" command implementation
  -- The unit of timeout value changes from millisecond to second
  -- "locate" command without timeout specified will be interpreted a 500 second timeout
  -- "locate" command with timeout 0 would bring the device out of locating state
  -- Device will quit locating state on a short press of ID button if it has been in locating state
- Fixed issue: HControl Secure mode setting doesn't persist over power cycle
- Fixed issue: Network address mode always displays as "Static" in Manager discovery page, even if in DHCP mode

----------------------------------------------------------
Known Issues
----------------------------------------------------------

- In DHCP, domain suffix may not populate when queried
- DNS entries currently limited to two (2).
- When setting digitalinputHighMin or digitalinputLowMax with float, a response may contain a redundant \x000
