
Last Updated: February 25, 2025


Product Name: N-Able
FG #: N-ABLE-PC

 
Version: 5.1.77
Release Date: 2025-02-25

-----------------------------------------------------------
Prerequisites
----------------------------------------------------------
**Starting in release 2023-09-03, SVSI V-Series is NO longer supported.


----------------------------------------------------------
Known Issues
----------------------------------------------------------



----------------------------------------------------------
Revision History
----------------------------------------------------------

Version 5.1.77
- Added a Syslog server option to allow for capture of device Syslog settings.

Version 5.1.73
- Added a H26x Firmware Column.
- Enhanced functionality of the HControl field. Double-click the HControl ID wanting to be changed a pop-up will open. Type the new name and press ok.
If you wish to reset the HControl name, send no name to the device by deleting the text and pressing OK. Only letters, numbers, and - are allowed
to be sent. Press Auto Discover after setting all the names to force a refresh of the HControl information. 

Version 5.1.71
- Enhanced performance during firmware updates

Version 5.1.69
- A column called "HControl" was added. This will display the device's HControl ID. To refresh/discover these values, press the Auto Discover
under the Unit Management Tab.
- Stability enhancements

Version 5.1.66
- Updated USB2 matrix to allow for up to 4 decoders to be routed to a single encoder of N2600
- Added a "Enable Select All" setting preference that will give the ability to route a single encoder to all decoders in a column. 

Version 5.1.63
- Enhanced the EDID Configuration tool
- Enhanced image preview. N-Able will disable image preview at 100 or more units and throttle updates at 100 or more. 
- Updated a firmware field to unit management displaying the primary version and H26x if dealing with N2600S units
- Updated switch all has been removed from the matrix removed
- Updated Firmware Updater by removing the Factory Restore option. If needed, the user can use the batch config to factory restore units.
- Stability enhancements


Version 5.1.52
- Stability enhancements
- Performance enhancements

Version 5.1.44
- Enhanced the dark mode function.
	automatically switches based on theme set in Windows
- Stability Enhancements	

Version 5.1.42
- Enhanced N2600 and N2600S auto-login method
- Enhanced KVM the matrix compatibility
- Enhanced the dialog when needing to send firmware from outside the subnet detected
- Enhanced the installer when loading on Windows 11 with a new VS Redist. package
- Fixed an issue with time zone and firmware compatibility checks
- Fixed an issue with the multicast discovery method

Version 5.1.31
- Enhanced N3300 auto-login method

Version 5.1.29
- Enhanced N3300 Series switching
- Fixed an issue with the Audio Switching Matrix

Version 5.1.27
- Added stability measures when updating the N1k and N2k products

Version 5.1.26
- Stability Enhancements

Version 5.1.22
- Added the ability for N2612S devices in Dual Stream mode to show both streams in the Video Matrix
- Added the routing capability of N2612S H26x stream to N2622S
- Stability Enhancements

Version 5.1.7
- Stability and Security Enhancements

Version 5.1.6
- Changed from a Date Version to a Numerical Version
- Added the N3300 Series
- Stability and Security Enhancements

Version 2023-09-21
- Removed the "Document" tab in the menu bar

Version 2023-09-03
- Performance enhancements

Version 2023-08-13
- Updated the ability to deploy firmware when units are in secure mode
- Condensed the video matrix to a single grid showing all N-Series units
- Added the ability to create Groups of different encoders/decoders
- Added a software audio decoder for troubleshooting
	- Audio must not be encrypted to be heard on the computer
- Added .svsiupdate formatting to the updater
	- allows for the .bin and .ver files to be condensed into a single file for 
	  management purpose of files.
- Added the ability to see both digital input resolutions on the N2600 Series Enc
- Added a firmware field in Unit Management
- Modified the Menu of Tools
- Added a Troubleshoot menu

Version 2023-04-04
- Performance enhancements
- Added "Select All" to Updater
- Fixed issue with displaying Resolutions on N2600 Series in Unit Management

Version 2022-12-21
- Performance enhancements
- Fixed missing elements in the settings pages of N-Series units

Version 2022-06-10
- Implemented row numbers into the unit management tab.

Version 2022-05-13
- Corrected issue with UnitDiff working with the N2300 Series
- Corrected issue when accessing N-CMD units not directing to HTTPS webpage

Version 2022-03-07
- Performance enhancements
- Allowing for increased firmware package size uploads
- Added CSV export/import of NetLinx menu items

Version 2021-12-13
- Added AES67 to import and export
- Improvements to the CSV menu items
- Improvements to the NVR panel
- Performance Enhancements

Version 2021-11-14
- Upgrade to the built-in web browser
- Mac version is back
- N-Able comes with built-in SSL support
- HDCP support is now available for all series by default
- Dark Mode
- Various rewordings... KVM Matrix, HDCP Settings, Menu, CSV export chooser has spaces
- Updater is now a Tool inside N-Able, and it has its own list of improvements
- Significant performance improvement to the unit management table
- Polling pausing at 50+ units has been removed
 

Version 2020-07-29
- Added AES67 Switching to SVSI products with current AES67 support.
- Added AES67 disabling when switching to SVSI audio stream.


Version 2018-01-29
- CSV performance and stability improvements
- Unit diff tool
- AES67 matrix improvements
- USB matrix improvements
- Documents browser app
- 2400 WP support

