Release Notes

Products: JPK-1300-UA, JPK-1300-EK
Description: AMX Jetpack Kit includes Receiver, Wallplate Transmitter, and Keypad
FG#: AMX-VTK0001 (US and Asia)
     AMX-VTK0001EK (Europe and UK)

File Name: SW_AMX-JPK-1300_v1.04.07.bin
Release Date: 3/4/2025
Firmware Version: V1.04.07

   - Receiver(RX):  V1.04.07
   - Wallplate(TX): V1.01.11
   - Keypad：        V1.01.08
   - Web：           V1.00.30


1. Prerequisites 
2. Features added in this release
3. Fixes in this release:  
4. Known Issues  
5. Programming Information  
6. Notable Points  

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
- Requires v1.03.10 or later to update

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
FW and Webgui
 - Added unsolicited feedback for System On/Off consistent with other async feedback
  -- "set device system on" response for System On (keypad or webgui button pressed)
  -- "set device system off" response for System Off (keypad or webgui button pressed)
  - Note the above is only the async responses to the button presses.  The "get system" 
    query has different unique responses as specified in the manual or telnet help.
 
 - Increased RS-232 Power On/Off Display Delay from 2000ms to 60000ms to allow more time
   between commands for certain situations 

Features in previous 1.04.06
 - None

Features in previous 1.04.04
FW and Webgui
 - Added IR Volume control option and IR Volume Up/Down learning. This allows control of the 
   connected HDMI display when using the keypad knob or API commands to set volume or mute. 
 - Added Daylight Saving Time feature.
 New feature settings are persisted to the config.json file
 Note: See instruction manual for details on new commands. See Webgui pages for updated features.

----------------------------------------------------------
3. Fixes in this release:
----------------------------------------------------------
MCU fix
 - Fixed Auto Display Off Delay Time so that it works correctly for delays greater than 10 minutes
   Note: There is approximately 15 sec of delay for signal loss detection before this Auto timer starts
 
Fixes in previous V1.04.06
MCU fixes
 - Improved IR Learning function for better compatibility with more devices.
 - Corrected issue where extra bytes were being appended to the IR code when pressing "Save"
 - Fixed logic issue in scheduling events to ensure that if DISPLAY ON action is scheduled, it will trigger, 
   regardless of whether there is an active input signal.
 - Corrected internal issue where ODD/EVEN Parity bit was inverted.  
   NOTE: If you previously had to select ODD (when EVEN was required by your display) and you load this FW, 
   then you will need to flip that back since the parity inversion is now corrected.
 - Optimized the serial port to not respond to ANY peripheral feedback/commands from externally controlled
   device when JPK-1300 is in RS-232 HOST mode.
   Note: Use Client mode to send serial commands to the JPK-1300 from an external controller/PC.
 - Solved the problem that when the configuration is imported, the serial port command is displayed but there 
   is no actual command output

Webgui fixes
 - Updated Factory Default pop-up text for clarity
 - Upgraded dropbear SSH client to version 2022.83

Fixes in previous V1.04.04 
 - None
 
Fixes in previous V1.04.03
 - Optimized Webgui Reboot feature so it will restart in the login interface automatically
 - Resolved Save/Load config problem causing serial port commands to not be exported/imported 
   properly in ASCII

Fixes in previous v1.04.02
Webgui
 - Clarify the private key supported format (both .key and .pem) for HTTPS certificate on the Webgui

FW
 - Fix feedback issue on Telnet/SSH when pressing either the “SOURCE” button on the Wall-plate TX
   or pressing “HDMI 1”, “HDMI 2” and “USB-C” button on the keypad

Fixes in previous V1.04.01
MCU
 - Optimize time zone setting related operations

Webgui
 - Fixed the time format
 - Disable Time Zone function and optimize logic when Set Time Automatically is set to OFF
 - Corrected an issue where saving the Schedule did not notify user if the save was successful

FW
 - Fixed issue where the product would not get the IPv6 address assigned by IPv6 server
 - Fixed audio/video issue when switching output mode between "sharing the screen" and "Samsung DEX" 
   using Type-C channel

API
 - Fixed "set dns" command
 - Corrected the IPV6 Mask Prefix (aka. Subnet Prefix Length) received from the API command "get ipv6" 
   to properly match the Webgui value

----------------------------------------------------------
4. Known Issues
----------------------------------------------------------

 - IMPORTANTE: After upgrading the firmware, it is best to perform a factory reset, to make sure any new or 
   updated parameters will get properly initialized

----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
 - USB2.0 SPDIF Audio requires 8 sec to be detected by USB-C Source when using USB2.0 Type-C to Type-C cable
 - Below is a summary to get Video and full functionality of Jetpack USB-C (DisplayPort, KVM and SPDIF Audio over USB2.0)
  -- For USB Type-C Video: The cable and source must support "DP Alt Mode"
  -- For USB-C Cable: Jetpack supports a maximum AV date rate up to 10Gbps (4K60:420 or 4K30/444), so the data transport
     rate of the cable needs to support up to 10Gbps.
   --- Based on DP Alt Mode for USB-C standard, USB-C Cable need compliant to:
   --- USB3.1 Gen1 (Equal to USB3.0) – 5Gbps (Lowest requirement to get full-feature of Jetpack USB-C connection)
   --- USB3.1 Gen2 – 10Gbps (Recommend requirement to get full-feature of Jetpack USB-C connection)
   --- Or higher version