##########################################################

            About Si Impact V1.7 build 10

##########################################################

New Features: 


Bug Fixes:

	Improved HiQnet discovery for connection robustness (delays HiQnet discovery slightly)
	Optimised filtering of non-ip protocol network traffic


Documentation:
* There is no documentation update for V1.7 software.
	

##########################################################

Software Update Instructions for Si Impact V1.7 build 10

##########################################################

01. Unzip the files to a USB key in the root directory, you should have two files:
	Impact.bin
	info.xml

02. Switch the console off using the POWER switch located on the rear of the console.

03. Press and hold the BOOT LOADER switch on the rear of the console for approx 5 seconds whilst you turn the console on. A SOFTWARE LOADER screen will appear.

04. Insert the USB stick and then press the MENU key.

05. If the fader firmware requires updating this will be prompted on the touch screen; 
	follow on-screen instructions for this process.
 
06. Select the INFO.XML file using the scroll/adjust encoder, the LOAD button at the bottom right
	of the touch screen window will appear when a valid selection is made.

07. Press the LOAD button. Software will begin loading.

08. Wait until both progress bars have reached 100%, and the 'tick' symbol has appeared
	to the right of each progress bar, before removing the USB stick.

NOTE: Always follow on-screen instructions as the process may vary if the software
on your console is more than 1 release old.

########################################################################

                CLEAR SD CARD (RESET TO FACTORY DEFAULT)

########################################################################

********************************IMPORTANT*******************************
Clearing the SD card will erase all files and settings on the console,
these must be backed up to a USB key before clearing the card or loading 
new software.
************************************************************************


CLEARING the internal SD CARD - THIS IS OPTIONAL WHEN INSTALLING V1.7 build 10

=============================================================================

The following procedure will restore the console to the factory defaults.

NOTE: All settings, cues, users, profiles and shows will be lost.

01. Starting with the console off, press and hold the BOOT LOADER switch on the rear of the console for approx 5 seconds whilst you turn the console on.

02. Press the MENU key once the loader screen appears.

03. Press the LR, MONO and FX1 keys together, this opens the update page.

04. Press the CLEAR SD CARD button on the touch screen.

05. Restart the console.

