Product Name: N-Series N1x22 Video Encoder/Decoder
FG #: FGN1122-SA (NMX-ENC-1122)
      FGN1222-SA (NMX-DEC-1222)
      FGN1122-CD (NMX-ENC-1122-C)
      FGN1222-CD (NMX-DEC-1222-C)
      
Version: v1.14.11e
Release Date: 07/20/2017

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- None

----------------------------------------------------------
2. Revision History
----------------------------------------------------------
Version 4/03/2017 (v1.14.11e - 7/20/2017)
•	Added new Panasonic PCT2485 touchscreen firmware support (see known issues)
Version 4/03/2017 (v1.14.11d)
•	Netlinx getStatus formatting fix
Version 4/03/2017 (v1.14.11b)
•	Correct time synchronization handling 
Version 4/03/2017 (v1.14.11)
•	Netlinx - Correct display of Svsi devices in Netlinx master webpage
•	Netlinx - Correct handling of 1024 byte buffered RS-232 Rx data
•	Netlinx- add VIDOUT_ON-[ON/OFF], modify VIOUT_MUTE to send/disable avmute
•	Netlinx- correct truncation of getStatus API response.
•	Increase KVM report size for Sharp touchpanel
Version 12/13/2016 (v1.13.6)
•	Improved monitor and display support support
•	Audio input is initialized to 48 kHz
•	Added support for Panasonic touch panel
•	HDMI 2.0 video source compatibility improvements.
•	Various fixes
Version 12/13/2016, Web: 12/28/2016 (v1.13.6b)
•	NetLinx 0.0.22: Netlinx fix to problem with the incorrect system number in a response to a STRING command.
Version 12/13/2016, Web: 12/29/2016 (v1.13.6c)
•	NetLinx 0.0.23: Bug fix
Version 12/13/2016, Web: 01/06/2017 (v1.13.6d)
•	NetLinx 0.0.24: Bug fix

----------------------------------------------------------
3. Known Issues
----------------------------------------------------------
•	Later built Panasonic PCT2485 touchscreens must be connected and powered before powering up decoder or the USB connection will hang until decoder rebooted.  Powering up both units at the same will also work.


