Release Notes

DVX-2100HD-SP-T 

FG#:   FG1905-01, FG1905-04 (DVX-2100HD-SP)
       FG1905-02, FG1905-05 (DVX-2100HD-T)

Current Firmware Version: v3.53.453
Release Date:03/02/2011

Device ID: 00000: (Master controller)
           05001: (NI device)
           05002: (DVX-2100HD-SP/T Switch)


----------------------------------------------------------
Dependencies
----------------------------------------------------------

Requires NI-Device firmware version of 1.30.8 or greater to fully utilize the enhancements. 
If NI-Device version 1.30.8 or later is loaded before this master firmware version, the 
integrated device (5001) will be unavailable until the master side firmware is upgraded. 

----------------------------------------------------------
Changes in this release
----------------------------------------------------------

- Added the ability to disable IP Device Discovery on the Network Settings Web page.
- Added Mio R3, AVX-400, and NXA-PDU-1508-8 Axlink types
- Removed erroneous "no help found" message from terminal "help security" request
- Fixed Telnet "set duet" command to support setting Duet memory greater than 99 for the new NI-X100/256
- Fixed an issue that could result in the integrated device (5001) reverting to a dynamic device number upon reboot.
- Fixed an issue that could result in master lockup when using ZeroConfig.
- Fixed an issue that could result in master lockup during MVP-9000i Ethernet Hot Swap.
- General stability improvements that prevent Master lockups under certain conditions.


----------------------------------------------------------
Known Issues 
----------------------------------------------------------
  
None

----------------------------------------------------------
Programming Information
----------------------------------------------------------

None
