Release Notes

DXLink 4K HDMI Receiver Module

FG#: FG1010-510 (DX-RX-4K)


Firmware Version: v2.1.74
Release Date:     05/24/2016

README.TXT File Contents

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Known Issues
5. Programming Information
6. Notable Points


----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- For directly connected MFTX Transmitters, the MFTX Transmitters must use firmware version 
  v1.8.24 (or later).

- For directly connected Solecis Transmitters, the Solecis Transmitters must use firmware version 
  v1.4.9 (or later).

- For connecting to Enova DGX 100 Series enclosures over DXLink, the Enova DGX will need the following FW versions:
    - For Enova DGXs with NX Masters: Enova DGX NX Master FW v1.4.86 (or later).
    - Enova DGX 800/1600/3200/6400 FW  v3.1.17 (or later).


- NetLinx Studio NetLinx Studio V3.4 (4.0 if using NX master)

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------
- Initial LR Release


----------------------------------------------------------
3. Fixes in this release: 
----------------------------------------------------------
- Initial LR Release


----------------------------------------------------------
4. Known Issues
----------------------------------------------------------


----------------------------------------------------------
5. Programming Information
----------------------------------------------------------
- The FPGA portion of the KIT file firmware download can take up to 10 minutes in itself. Please be patient during upgrades.


----------------------------------------------------------
6. Notable Points
----------------------------------------------------------
- PLEASE READ the documentation in regard to the DIP switches located on the DXLink 4K HDMI Receiver Module
  before attempting to connect to the network.
