Release Notes

DXLink HDMI Receiver Module Firmware
(Enova DGX 100 Series Compatible)

!!IMPORTANT:  READ PROGRAMMING INFORMATION SECTION BELOW 
IN REGARD TO UPGRADING OLDER FIRMWARE VERSIONS!!

!!This firmware version requires Enova DGX 100 Series
compatibility on connected Enova DGX systems!!

!!!Please reference the Enova DGX Board and Endpoint
Compatibility Instructions on the AMX.com product
page for more information!!!

FG#: 
  FG1010-500 (DX-RX, DXLink HDMI Receiver Module)

Release Date: 06/03/2016
Current Released Firmware: v1.13.28
SW1010_500_AVB_KIT_DXLINK_RX_v1_13_28.kit


----------------------------------------------------------
Table of Contents
----------------------------------------------------------

1. Prerequisites
2. Features added in this release
3. Fixes in this release:
4. Notable Points
5. Programming Information

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- DXLink RX v1.9.10 (or later) must be loaded on the DXLink 
  Receiver to upgrade

- DXLink TX v1.8.26 (or later) must be used on the DXLink 
  Receiver for best performance with this RX version

- Enova DGX 800/1600/3200/6400 must have v3.2.4 (or later)
  to allow use of the new ICSLAN feature and async status
  improvements in this release. Else v3.0.20 (or later)
  The DGX 100 Series Master FW should be:

    - SW2106_NX-X200_Master_v1_4_86.kit(or later)

- Enova DGX 8/16/32/64 enclosures need Enova DGX 8/16/32/64
  FW v2.2.8 (or later) and Master FW:

    - SW1056_Master_v4_2_395.KIT or later (NI-Series)
      Shows in Online Tree as "NI Master"

    - SW2106_NX-X200_Master_v1_3_110.kit or later (NX-Series)
      Shows in Online Tree as "DGX Master"

- NetLinx Studio v4.3.1519 or later

- DGX Configuration Software v1.0.6 or later

----------------------------------------------------------
2. Features added in this release:
----------------------------------------------------------

- Added ability to set RX ICSLAN port to be on the public
  or private network. Added new DGX ICSP command:
  5002:y:0 ENDPOINT_RX_ICSLAN_PORT-<PRIVATE|PUBLIC>
  Where y is the input channel connected to the RX.
  !!NOTE: This requires DGX v3.2.4 (or later)!!

----------------------------------------------------------
3. Fixes in this release: 
----------------------------------------------------------

- Fixed an issue on RX where a DGX reboot could cause an
  HDCP failure and Orange Screen on certain displays

- Improved HDCP data management to prevent false HDCP flag 

- Fixed an issue where the RX goes offline when using 232
  control of Sharp LC60LE661U (or similar models)

- Improved handling of audio async messages 

- Corrected an issue where spurious interrupts could cuase
  the RX to drop offline

- Fixed IR one way serial reliability at 9800 baud

- Fixed VIDOUT_SLEEP_DELAY when set to zero. Now a value of 
  zero will allow the RX to sleep immediately with no video

- Improved reliability of Audio Valid flag setting in Audio 
  details

----------------------------------------------------------
4. Notable Points
----------------------------------------------------------

- Please read the documentation in regard to the DIP
  switches located on the bottom of the Tx/Rx modules
  before attempting to connect to the network.

- If a send command "FACTORYAV" or telnet "RESET FACTORY" 
  is sent, a reboot of the RX will be required.

- PLEASE READ the documentation in regard to the DIP 
  switches located on the bottom of the Tx/Rx modules 
  before attempting to connect to the network

- The RX uses a solid ORANGE screen to indicate an HDCP 
  authentication failure with the connected device 

- If using a hostname in the USB_HID_ROUTE command, the 
  hostname length is limited to 50 characters

----------------------------------------------------------
5. Programming Information
----------------------------------------------------------

!! IMPORTANT: Scaler settings upgrade migration
!!
!! If upgrading to DGX from v3.0.10 to any later version
!! and if DXLink RX are configured with non-default scaler
!! settings (scaling mode, aspect ratio and manual res/ref),
!! the "PERSISTAV" ICSP command should be sent to those RX's
!! before upgrading either the DGX or the RX's in order to 
!! preserve their modified scaler settings.

--UPGRADING-----------------------------------------------
!! Important–Due to a HWID change, this kit will FAIL on!!
!! the first attempt of the kit transfer IF upgrading   !!
!! from firmware earlier than v1.9.32                   !!
!!                                                      !!
!! 1. Transfer kit v1.13.28 to the RX. If upgrading from!!
!!    a version earlier than 1.9.32, it will abort:     !!
!!    "Transfer Aborted - Unsupported file type."       !!
!!    If this happens, then proceed to step 2           !!
!!                                                      !!
!! 2. Reboot the RX (via telnet or power cycle) then    !!
!!    check the firmware versions in the Online Tree:   !!
!!                                                      !!
!!eg. 07001 - DXLINK-HDMI-RX.e (v1.13.28)               !!
!!      [OID=1] - MQX (v3.62)                           !!
!!      [OID=2] - DXLINK Boot (v1.13.28)                !!
!!      [OID=3] - DXLINK App (v1.13.28)                 !!
!!      [OID=5] - DXLINK Link (3.0.6.0)                 !!
!!      [OID=6] - DXLINK FPGA (1.0.0.6)                 !!
!!                                                      !!
!! 3. If the firmware versions are not up to date, then !!
!!    transfer kit v1.13.28 again to completele the     !!
!!    transfer of the final components. If the firmware !!
!!    has updated, no other kit transfers are required. !!
==========================================================

- PLEASE reference Appendix A (Upgrading the Firmware) in the 
  DXLink Instruction Manual for more information.
