Product Name: MVP-9000i - 9" Modero ViewPoint Wireless Touch Panel with Intercom

FG#: FG5967-01 (MVP-9000i black)
     FG5967-02 (MVP-9000i white)

Current Firmware Version: 2.86.86
Release Date: 2/4/2015
Device ID: 0x157

Prerequisites: 
Master FW capable of hotswapping build 439 or later
TPDesign4 3.0 build 634 or later.
Intercom module v1.9 or later.
SIP module 2.11 or later
TDS/WDS Firmware 1.10.6 or later

Changes in this release
-----------------------
-- Fixed issue with the flyout buttons on the left side of the front panel. 
   The panel will appear to stall and possibly revert to the main startup page 
   if any of the four flyout buttons are pressed after a bootup but before the
   capacitive touch pad on the right side of the front panel is pressed.
-- Fixed a SIP registration issue where registration with some SIP proxies 
   would fail if the proxy was unable to accept an "expires" value of 180 
   seconds. An "expires" value of 3600 is now the default.
-- Fixed a SIP issue where cycling the SIP state between enabled and disabled 
   could sometimes cause the panel to get stuck in a state where it could no 
   longer register with the proxy until the panel was rebooted.
-- Fixed issue where user was unabled to enter setup pages by holding their
   finger on the screen during boot.
-- Fixed issue with a channel assigned to the cradle sensor getting out of sync
   after a reboot.
-- Fixed issue where motion jpeg images would not display if the server rejected
   HTTP/1.0 requests.
-- Fixed issue where the dock sound would play any time the panel became 
   disconnected from the master.
-- Updated WiFi firmware to conform to R&TTE adaptivity requirements described  
   in the ETSI R&TTE EN 300 328 v1.8.1 standard.

Known Issues
------------
DOCK AND UNDOCK:
-- If a panel is docked, any loss of network connectivity on the wired 
   interface (such as a connected switch going down) may lead to unexpected 
   issues like one way voice or inability to connect to remote servers 
   (e.g. for SIP, dynamic images).
-- If the wired interface will not be used (in other words, the docking 
   station is being used for storage and charging only), the Wired network 
   settings should be left at their factory defaults (DHCP).

TABLE DOCK LATCH:
-- When the panel is removed from a dock with the Table Dock Latch set to "off" 
   it will take longer for the panel to reconnect wirelessly than usual.  The 
   panel waits for the master to timeout the device number, and then reconnects 
   to the master with the same device number.  With non-encrypted ICSP, the 
   panel disconnects and reconnects to a master in about 3-4 seconds.  Encrypted   ICSP will take around 15-20 seconds to reconnect. It is recommended not to 
   use wired ethernet if the panel is set to forced undocks to avoid the 
   transition time between wired and wireless modes.

USB:
-- TPD4 file with wrong resolution can be downloaded.
-- OTG USB host is sometimes not recognized upon plugging in. Unplugging and 
   replugging should fix.

POWER MANAGEMENT:
-- Sleep cannot be disabled and a non-zero value for sleep timeout must be set.    The default value is the maximum value of 2 hours.
-- The panel cannot enter full standby mode if there is a USB device plugged 
   in or MicroSD card inserted.

INTERCOM AND DYNAMO:
-- When the panel is connected wirelessly (particularly with a weak signal) 
   and streaming audio and video with a MET-ECOM, the video rate may slow to a 
   few frames per seconds.  This can cause the MET-ECOM to send bad frames 
   which can lead to occasional video freeze and one-way or no audio.

IP:
-- If a Static IP is set on the wired (or wireless) settings in the same 
   subnet range as the USB (172.16.x.x), the gateway populates with 
   255.255.255.255. This is only cosmetic and does not impact the performance

WIRELESS:
-- The roaming/band changes may cause the panel roaming settings to change 
   during the upgrade process, double check the roam settings after upgrading 
   if you are using active roaming.

PROGRAMMING INFORMATION:
-----------------------
After upgrading you MUST resave wireless settings.  You do not have to reenter 
the settings.  Open wireless page and press save.

Band Selection: Note - The band selection will effect what you see when doing 
a site survey.

802.11a/b/g -> A and B bands, all channels
802.11b/g -> B band, channels 1,6,11
802.11a -> A band, all channels

Active roaming:
Disabled -> Roaming is passive, and will only occur when the panel loses 
connection to its current access point Enabled -> The panel is actively 
looking for better access points to roam to.
