Product Name: 
	NXx-1200V   Modero 12" Active Color Touch Panel with video
	NXx-1200VG  Modero 12" Active Color Touch Panel with video/RGB
	NXx-1500VG  Modero 15" Active Color Touch Panel with video/RGB
	NXx-1700VG  Modero 17" Active Color Touch Panel with video/RGB

FG#: 
	FG2250-60	
	FG2251-60
	FG2250-61
	FG2251-61
	FG2252-61
	FG2253-61
	FG2256-61
	FG2257-61

Current Firmware Version:
	2.86.23

Release Date: 
	09/14/10

Device Id:
	x013E
	x013F
	x0140
	x0141
----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------
	None

----------------------------------------------------------
2. Firmware Revision History
----------------------------------------------------------
Boot:
-- Delay added to boot to meet spec for large compact flash cards.

User Interface:
-- New touch calibration algorithm which provides more accuracy and
   corrects for nonlinear error in the touch overlays. The new algorithm
   adds more points to the touch calibration.

Setup Pages:
-- Added new calibration page compatible with the new touch calibration.

----------------------------------------------------------
3. Known Issues - 
----------------------------------------------------------
-- When downgrading from 2.86.xx or later to a version of 2.85.xx or
   earlier a reset of the system settings is required.

-- When connecting to the panel via USB (i.e. firmware transfer,
   panel file download, telnet, etc) the cable should be
   disconnected *before* a reboot.  If it is still connected
   there is a small possibility that the panel will boot and
   detect a USB issue and reboot again.  This reboot cycle
   will continue, never leaving the splash screen, until the
   panel is power cycled or shutdown.  This is not a new problem.
   It has been an issue with the manufacturers USB driver for
   many years.  However, previously the panel would just hang
   on the splash screen and the panel would require a power
   cycle.  Because we have made things more robust we now try to
   reboot the panel whereas before we did not.  Thus, the error
   does not get cleared and the reboots continue.  A simple power
   cycle or shutdown using the external buttons will clear this issue.

----------------------------------------------------------
4. Programming Information
----------------------------------------------------------
Important:    Panels with more than 1Gb Compact Flash cards should not be 
              downgraded to any version below 2.86.20.  This information can be
              retrieved via Setup pages (Information - File System), or using telnet - (disk free).