NXV-300 (FG2263-01) Build v2.1.25 Release Notes
----------------------------------

Build Date: 9/8/2015

Prerequisites
-------------
None

Changes in this release
-----------------------
-- The FTP server port is closed to enhance security.

-- Updated the CA (certificate authority) for the VNC (vncviewer.jar) Java 
   package.

Known Issues
------------
-- It is observed that in page tracking mode, when the "Sleep" button 
   (with "0-loop back port") of the NXV-300 is clicked using the USB mouse, 
   the NXV-300 may switch between sleep mode and wake mode. This 
   feature also appears to cause other panels connected to the same master to 
   permanently go to into sleep mode.

-- The master settings are still applied even though the "Cancel" button in 
   "System Settings" page was pressed. 

-- It is observed that either doing a "Reset System Settings" in the 
   "Protected Setup" page or downloading the full kit to the NVX-300 in 
   480x272 resolution, the NVX-300 boots up with 800x480 resolution.

-- The text "Bonjour" is missing in the "Device Name" alpha numeric keyboard 
   in the Title position.

-- The display timeout feature is not available. 

-- The "Connect Count" in the "G4 Web Control Settings" page is not reliable.

-- The Protected Setup page "Password" is not case sensitive when it is 
   entered using Desktop "Keyboard".

-- The Connection Status Symbol shows up in red color when the NXV-300 
   connects in URL(UDP) or NDP(UDP) while in DHCP mode, even though Netlinx 
   Studio shows that it is connected to the master.
