<?xml version="1.0" encoding="UTF-8" standalone="yes" ?>

<P3Model xmlns="p3.martin.com" ManufacturerId="19792" SeriesId="26" ProductId="00" RDMDeviceModelID="215" ArtNetOEMCode="11852">
    <Name>MAC Encore Two</Name>
    <ShortName>MAC Encore Two</ShortName>
    <RangeName>MAC</RangeName>
    <SeriesName>MAC Encore Series</SeriesName>
    <Category>Fixture</Category>
    <Checksum>f124c59e 2ccfa3ce 0bfd136e 7987876b 2ac1f85f</Checksum>

    <PhysicalProperties>
        <Dimensions>
            <HorizontalPixelPitch>24</HorizontalPixelPitch>
            <VerticalPixelPitch>24</VerticalPixelPitch>
        </Dimensions>

        <OutlineShape>Circle</OutlineShape>

        <OneToOnePixels>
            <Outline width="8" height="8"/>
            <pixel x="-1"  y="-1"/>
            <pixel x="1"  y="-1"/>
            <pixel x="1"  y="1"/>
            <pixel x="-1"  y="1"/>
            <pixel x="3"  y="0"/>
            <pixel x="-3"  y="0"/>
        </OneToOnePixels>

        <RealWorldPixels>
            <Outline width="146.00000000" height="146.00000000"/>
            <pixel x="-14.600000"   y="-25.287942"/>
            <pixel x="25.287942"   y="-14.600000"/>
            <pixel x="14.600000"   y="25.287942"/>
            <pixel x="-25.287942"   y="14.600000"/>
            <pixel x="58.400000"   y="0.000000"/>
            <pixel x="-58.400000"   y="0.000000"/>
        </RealWorldPixels>

        <Shape>FreePixel</Shape>
        <ReferencePixel>0</ReferencePixel>

        <ColourCalibration FeatureId="5" />
        <!-- Direct Color -->
    <!--    <ColourTargets  EnumVal="0"  OutputUnit="lm">--> <!-- Data Supplied by R&D -->
    <!--        <White Output="21000" x="333" y="345"/>-->
    <!--        <Red   Output= "1814" x="687" y="310"/>-->
    <!--        <Green Output= "1002" x="115" y="774"/>-->
    <!--        <Blue  Output=  "189" x="159" y="21"/>-->
    <!--    </ColourTargets>-->
        <!-- Calibrated Color -->
    <!--    <ColourTargets  EnumVal="1"  OutputUnit="lm">--> <!-- Data Supplied by R&D -->
    <!--        <White Output="21000" x="333" y="345"/>-->
    <!--        <Red   Output= "1812" x="688" y="309"/>-->
    <!--        <Green Output= "1008" x="116" y="770"/>-->
    <!--        <Blue  Output=  "252" x="162" y="26"/>-->
    <!--    </ColourTargets>-->
        <!-- Extended Gamut -->
    <!--    <ColourTargets  EnumVal="2"  OutputUnit="lm">--> <!-- Data Supplied by R&D -->
    <!--        <White Output="21000" x="333" y="345"/>-->
    <!--        <Red   Output= "1808" x="688" y="309"/>-->
    <!--        <Green Output=  "995" x="111" y="779"/>-->
    <!--        <Blue  Output=  "187" x="158" y="20"/>-->
    <!--    </ColourTargets>-->

        <MaxAmbientTemperature>90</MaxAmbientTemperature>
        <DefaultThermalThrottlingStart>80</DefaultThermalThrottlingStart>

        <ColourDepth>16</ColourDepth>

        <EthernetPorts>
            <EthernetPort Speed="100"/>
            <EthernetPort Speed="100"/>
        </EthernetPorts>
    </PhysicalProperties>

    <DMXModes ModeFeatureId="6" OverrideFeatureId="9" SupportsMultiUniverse="Yes" GDTFSpec="Martin_Professional@MAC_Encore_Two">
        <!-- Basic -->
        <DMXMode Value="0" GDTFMode="Basic" ChannelCount="52">
            <Channel Name="Strobe/Shutter" BitDepth="8"/>
            <Channel Name="Dimmer" BitDepth="16"/>
            <Channel Name="Cyan" BitDepth="16"/>
            <Channel Name="Magenta" BitDepth="16"/>
            <Channel Name="Yellow" BitDepth="16"/>
            <Channel Name="CTO" BitDepth="16"/>
            <Channel Name="CTC" BitDepth="8"/>
            <Channel Name="Tint" BitDepth="8"/>
            <Channel Name="Color Wheel" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Selection" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Index/Rotation" BitDepth="16"/>
            <Channel Name="Gobo Wheel 2 Selection" BitDepth="8"/>
            <Channel Name="Animation Insertion" BitDepth="8"/>
            <Channel Name="Animation Index/Rotation" BitDepth="16"/>
            <Channel Name="Frost 1" BitDepth="8"/>
            <Channel Name="Frost 2" BitDepth="8"/>
            <Channel Name="Prism Insertion" BitDepth="8"/>
            <Channel Name="Prism Index/Rotation" BitDepth="16"/>
            <Channel Name="Iris" BitDepth="8"/>
            <Channel Name="Zoom" BitDepth="16"/>
            <Channel Name="Focus" BitDepth="16"/>
            <Channel Name="Framing 1 Position" BitDepth="8"/>
            <Channel Name="Framing 1 Angle" BitDepth="8"/>
            <Channel Name="Framing 2 Position" BitDepth="8"/>
            <Channel Name="Framing 2 Angle" BitDepth="8"/>
            <Channel Name="Framing 3 Position" BitDepth="8"/>
            <Channel Name="Framing 3 Angle" BitDepth="8"/>
            <Channel Name="Framing 4 Position" BitDepth="8"/>
            <Channel Name="Framing 4 Angle" BitDepth="8"/>
            <Channel Name="Framing Rotation" BitDepth="8"/>
            <Channel Name="Pan" BitDepth="16"/>
            <Channel Name="Tilt" BitDepth="16"/>
            <Channel Name="Settings" BitDepth="8"/>
            <Channel Name="LED Frequency" BitDepth="8"/>
            <Channel Name="P3 Mix" BitDepth="8"/>
            <Channel Name="FX1" BitDepth="8"/>
            <Channel Name="FX1 Adjust" BitDepth="8"/>
            <Channel Name="FX2" BitDepth="8"/>
            <Channel Name="FX2 Adjust" BitDepth="8"/>
            <Channel Name="FX Sync" BitDepth="8"/>
        </DMXMode>
        <!-- Extended -->
        <DMXMode Value="1" GDTFMode="Extended" ChannelCount="62">
            <Channel Name="Strobe/Shutter" BitDepth="8"/>
            <Channel Name="Dimmer" BitDepth="16"/>
            <Channel Name="Cyan" BitDepth="16"/>
            <Channel Name="Magenta" BitDepth="16"/>
            <Channel Name="Yellow" BitDepth="16"/>
            <Channel Name="CTO" BitDepth="16"/>
            <Channel Name="CTC" BitDepth="8"/>
            <Channel Name="Tint" BitDepth="8"/>
            <Channel Name="Color Wheel" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Selection" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Index/Rotation" BitDepth="16"/>
            <Channel Name="Gobo Wheel 2 Selection" BitDepth="8"/>
            <Channel Name="Animation Insertion" BitDepth="8"/>
            <Channel Name="Animation Index/Rotation" BitDepth="16"/>
            <Channel Name="Frost 1" BitDepth="8"/>
            <Channel Name="Frost 2" BitDepth="8"/>
            <Channel Name="Prism Insertion" BitDepth="8"/>
            <Channel Name="Prism Index/Rotation" BitDepth="16"/>
            <Channel Name="Iris" BitDepth="16"/>
            <Channel Name="Zoom" BitDepth="16"/>
            <Channel Name="Focus" BitDepth="16"/>
            <Channel Name="Framing 1 Position" BitDepth="16"/>
            <Channel Name="Framing 1 Angle" BitDepth="16"/>
            <Channel Name="Framing 2 Position" BitDepth="16"/>
            <Channel Name="Framing 2 Angle" BitDepth="16"/>
            <Channel Name="Framing 3 Position" BitDepth="16"/>
            <Channel Name="Framing 3 Angle" BitDepth="16"/>
            <Channel Name="Framing 4 Position" BitDepth="16"/>
            <Channel Name="Framing 4 Angle" BitDepth="16"/>
            <Channel Name="Framing Rotation" BitDepth="16"/>
            <Channel Name="Pan" BitDepth="16"/>
            <Channel Name="Tilt" BitDepth="16"/>
            <Channel Name="Settings" BitDepth="8"/>
            <Channel Name="LED Frequency" BitDepth="8"/>
            <Channel Name="P3 Mix" BitDepth="8"/>
            <Channel Name="FX1" BitDepth="8"/>
            <Channel Name="FX1 Adjust" BitDepth="8"/>
            <Channel Name="FX2" BitDepth="8"/>
            <Channel Name="FX2 Adjust" BitDepth="8"/>
            <Channel Name="FX Sync" BitDepth="8"/>
        </DMXMode>
        <!-- Ludicrous -->
        <DMXMode Value="2" GDTFMode="Ludicrous" ChannelCount="68">
            <Channel Name="Strobe/Shutter" BitDepth="8"/>
            <Channel Name="Dimmer" BitDepth="16"/>
            <Channel Name="Cyan" BitDepth="16"/>
            <Channel Name="Magenta" BitDepth="16"/>
            <Channel Name="Yellow" BitDepth="16"/>
            <Channel Name="CTO" BitDepth="16"/>
            <Channel Name="CTC" BitDepth="8"/>
            <Channel Name="Tint" BitDepth="8"/>
            <Channel Name="Color Wheel" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Selection" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Index/Rotation" BitDepth="16"/>
            <Channel Name="Gobo Wheel 2 Selection" BitDepth="8"/>
            <Channel Name="Animation Insertion" BitDepth="8"/>
            <Channel Name="Animation Index/Rotation" BitDepth="16"/>
            <Channel Name="Frost 1" BitDepth="8"/>
            <Channel Name="Frost 2" BitDepth="8"/>
            <Channel Name="Prism Insertion" BitDepth="8"/>
            <Channel Name="Prism Index/Rotation" BitDepth="16"/>
            <Channel Name="Iris" BitDepth="16"/>
            <Channel Name="Zoom" BitDepth="16"/>
            <Channel Name="Focus" BitDepth="16"/>
            <Channel Name="Framing 1 Position" BitDepth="16"/>
            <Channel Name="Framing 1 Angle" BitDepth="16"/>
            <Channel Name="Framing 2 Position" BitDepth="16"/>
            <Channel Name="Framing 2 Angle" BitDepth="16"/>
            <Channel Name="Framing 3 Position" BitDepth="16"/>
            <Channel Name="Framing 3 Angle" BitDepth="16"/>
            <Channel Name="Framing 4 Position" BitDepth="16"/>
            <Channel Name="Framing 4 Angle" BitDepth="16"/>
            <Channel Name="Framing Rotation" BitDepth="16"/>
            <Channel Name="Pan" BitDepth="16"/>
            <Channel Name="Tilt" BitDepth="16"/>
            <Channel Name="Settings" BitDepth="8"/>
            <Channel Name="LED Frequency" BitDepth="8"/>
            <Channel Name="P3 Mix" BitDepth="8"/>
            <Channel Name="FX1" BitDepth="8"/>
            <Channel Name="FX1 Adjust" BitDepth="8"/>
            <Channel Name="FX2" BitDepth="8"/>
            <Channel Name="FX2 Adjust" BitDepth="8"/>
            <Channel Name="FX Sync" BitDepth="8"/>
            <Channel Name="Engine Segment" BitDepth="8" Repeat="Yes"/>
        </DMXMode>
        <!-- Compact -->
        <DMXMode Value="3" GDTFMode="Compact" ChannelCount="46">
            <Channel Name="Strobe/Shutter" BitDepth="8"/>
            <Channel Name="Dimmer" BitDepth="16"/>
            <Channel Name="Cyan" BitDepth="16"/>
            <Channel Name="Magenta" BitDepth="16"/>
            <Channel Name="Yellow" BitDepth="16"/>
            <Channel Name="CTO" BitDepth="16"/>
            <Channel Name="CTC" BitDepth="8"/>
            <Channel Name="Tint" BitDepth="8"/>
            <Channel Name="Color Wheel" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Selection" BitDepth="8"/>
            <Channel Name="Gobo Wheel 1 Index/Rotation" BitDepth="16"/>
            <Channel Name="Gobo Wheel 2 Selection" BitDepth="8"/>
            <Channel Name="Animation Insertion" BitDepth="8"/>
            <Channel Name="Animation Index/Rotation" BitDepth="16"/>
            <Channel Name="Frost 1" BitDepth="8"/>
            <Channel Name="Frost 2" BitDepth="8"/>
            <Channel Name="Prism Insertion" BitDepth="8"/>
            <Channel Name="Prism Index/Rotation" BitDepth="16"/>
            <Channel Name="Iris" BitDepth="8"/>
            <Channel Name="Zoom" BitDepth="16"/>
            <Channel Name="Focus" BitDepth="16"/>
            <Channel Name="Framing 1 Position" BitDepth="8"/>
            <Channel Name="Framing 1 Angle" BitDepth="8"/>
            <Channel Name="Framing 2 Position" BitDepth="8"/>
            <Channel Name="Framing 2 Angle" BitDepth="8"/>
            <Channel Name="Framing 3 Position" BitDepth="8"/>
            <Channel Name="Framing 3 Angle" BitDepth="8"/>
            <Channel Name="Framing 4 Position" BitDepth="8"/>
            <Channel Name="Framing 4 Angle" BitDepth="8"/>
            <Channel Name="Framing Rotation" BitDepth="8"/>
            <Channel Name="Pan" BitDepth="16"/>
            <Channel Name="Tilt" BitDepth="16"/>
            <Channel Name="Settings" BitDepth="8"/>
            <Channel Name="LED Frequency" BitDepth="8"/>
        </DMXMode>
    </DMXModes>

    <MvrProperties>
        <MvrRotationType>YokeFixture</MvrRotationType>
    </MvrProperties>

    <ConfigurationOptions>
        <TestPatternControl FeatureId="3" NoneValue="0" WhiteValue="1" RedValue="2" GreenValue="3" BlueValue="4" OutlineValue="6" IntensityFeatureId="4"/>
        <IdentifyControl FeatureId="47" OffValue="0" OnValue="9"/>
        <DmxPatchControl AddressFeatureId="7" UniverseFeatureId="8"/>

        <Feature FeatureName="Fixture ID" FeatureId="00" NFCRecord="2" NFCOffset="12" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>1</RangeMin>
                <RangeMax>65535</RangeMax>
                <EncodeMin>1</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Serial Number" FeatureId="01" NFCRecord="1" NFCOffset="14" FeatureType="Label">
            <EncodeBytes>32</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="Firmware Version" FeatureId="02" FeatureType="Version"> <!-- P3 ONLY -->
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="Firmware Version" NFCRecord="1" NFCOffset="46" FeatureType="Label"> <!-- NFC ONLY -->
            <EncodeBytes>12</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="TestPattern Selection" FeatureId="03" FeatureType="Discrete"> <!-- P3 ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="[None]"/>
                <Enum EnumVal="1" EnumLabel="Mixed White"/>
                <Enum EnumVal="2" EnumLabel="Full Red"/>
                <Enum EnumVal="3" EnumLabel="Full Green"/>
                <Enum EnumVal="4" EnumLabel="Full Blue"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="TestPattern Intensity" FeatureId="04" FeatureType="Range"> <!-- P3 ONLY -->
            <Unit>%</Unit>
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>100</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>255</EncodeMax>
            </Range>
            <DefaultValue>255</DefaultValue>
        </Feature>

        <Feature FeatureName="Color Mode" FeatureId="05" NFCRecord="2" NFCOffset="31" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Direct Color"/>
                <Enum EnumVal="1" EnumLabel="Calibrated Color"/>
                <Enum EnumVal="2" EnumLabel="Extended Gamut"/>
            </EnumMap>
            <DefaultValue>2</DefaultValue>
        </Feature>

        <Feature FeatureName="DMX Mode" FeatureId="06" NFCRecord="2" NFCOffset="14" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Basic"/>
                <Enum EnumVal="1" EnumLabel="Extended"/>
                <Enum EnumVal="2" EnumLabel="Ludicrous"/>
                <Enum EnumVal="3" EnumLabel="Compact"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="DMX Address" FeatureId="07" NFCRecord="2" NFCOffset="0" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>1</RangeMin>
                <RangeMax>512</RangeMax>
                <EncodeMin>1</EncodeMin>
                <EncodeMax>512</EncodeMax>
            </Range>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="DMX Universe" FeatureId="08" NFCRecord="2" NFCOffset="2" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>1</RangeMin>
                <RangeMax>63999</RangeMax>
                <EncodeMin>1</EncodeMin>
                <EncodeMax>63999</EncodeMax>
            </Range>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="DMX Override" FeatureId="09" FeatureType="Discrete"> <!-- P3 ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Pan/Tilt Speed" FeatureId="10" NFCRecord="2" NFCOffset="21" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Fast"/>
                <Enum EnumVal="1" EnumLabel="Smooth"/>
                <Enum EnumVal="2" EnumLabel="Standard"/>
            </EnumMap>
            <DefaultValue>2</DefaultValue>
        </Feature>

        <Feature FeatureName="Effects Speed" FeatureId="11" NFCRecord="2" NFCOffset="22" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Follow P/T"/>
                <Enum EnumVal="1" EnumLabel="Fast"/>
                <Enum EnumVal="2" EnumLabel="Smooth"/>
                <Enum EnumVal="3" EnumLabel="Standard"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Effects Shortcuts" FeatureId="12" NFCRecord="2" NFCOffset="25" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Dimmer Curve" FeatureId="13" NFCRecord="2" NFCOffset="16" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Linear"/>
                <Enum EnumVal="1" EnumLabel="Square Law"/>
                <Enum EnumVal="2" EnumLabel="Inverse Square Law"/>
                <Enum EnumVal="3" EnumLabel="S-Curve"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Tungsten Emulation" FeatureId="14" NFCRecord="2" NFCOffset="43" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Focus Tracking" FeatureId="15" NFCRecord="2" NFCOffset="23" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Near"/>
                <Enum EnumVal="2" EnumLabel="Medium"/>
                <Enum EnumVal="3" EnumLabel="Far"/>
            </EnumMap>
            <DefaultValue>2</DefaultValue>
        </Feature>

        <Feature FeatureName="Gobo CT Correction" FeatureId="16" NFCRecord="2" NFCOffset="44" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Keylight Calibration" FeatureId="17" NFCRecord="2" NFCOffset="46" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Automatic"/>
                <Enum EnumVal="1" EnumLabel="Manual"/>
                <Enum EnumVal="2" EnumLabel="Disable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="FollowSpot Mode" FeatureId="18" NFCRecord="2" NFCOffset="33" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Video Tracking" FeatureId="19" NFCRecord="2" NFCOffset="17" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Reset via DMX" FeatureId="20" NFCRecord="2" NFCOffset="24" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Cooling Mode" FeatureId="21" NFCRecord="2" NFCOffset="32" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="4" EnumLabel="Constant Full"/>
                <Enum EnumVal="5" EnumLabel="Regulated High"/>
                <Enum EnumVal="6" EnumLabel="Regulated Medium"/>
                <Enum EnumVal="7" EnumLabel="Regulated Low"/>
                <Enum EnumVal="8" EnumLabel="Regulated Ultra Low"/>
            </EnumMap>
            <DefaultValue>5</DefaultValue>
        </Feature>

        <Feature FeatureName="Hibernation" FeatureId="22" NFCRecord="2" NFCOffset="112" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Offline Mode" FeatureId="23" NFCRecord="2" NFCOffset="73" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Run Stand-Alone Show"/>
                <Enum EnumVal="1" EnumLabel="Hold Last Look"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Stand-Alone Mode" NFCRecord="2" NFCOffset="74" FeatureType="Discrete"> <!-- NFC ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Individual"/>
                <Enum EnumVal="1" EnumLabel="Sync Host"/>
                <Enum EnumVal="2" EnumLabel="Sync Client"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Display" FeatureId="24" NFCRecord="2" NFCOffset="26" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="On"/>
                <Enum EnumVal="1" EnumLabel="AutoOff 2min"/>
                <Enum EnumVal="2" EnumLabel="AutoOff 5min"/>
                <Enum EnumVal="3" EnumLabel="AutoOff 10min"/>
                <Enum EnumVal="4" EnumLabel="Off"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="Display Intensity" FeatureId="25" NFCRecord="2" NFCOffset="27" FeatureType="Range">
            <Unit>%</Unit>
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>10</RangeMin>
                <RangeMax>100</RangeMax>
                <EncodeMin>10</EncodeMin>
                <EncodeMax>100</EncodeMax>
            </Range>
            <DefaultValue>50</DefaultValue>
        </Feature>

        <Feature FeatureName="Display Rotation" FeatureId="26" NFCRecord="2" NFCOffset="28" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Normal"/>
                <Enum EnumVal="1" EnumLabel="Rotate 180"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Display Contrast" FeatureId="27" NFCRecord="2" NFCOffset="29" FeatureType="Range">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>3</RangeMin>
                <RangeMax>100</RangeMax>
                <EncodeMin>3</EncodeMin>
                <EncodeMax>100</EncodeMax>
            </Range>
            <DefaultValue>41</DefaultValue>
        </Feature>

        <Feature FeatureName="Display Show Errors" FeatureId="28" NFCRecord="2" NFCOffset="30" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Normal"/>
                <Enum EnumVal="1" EnumLabel="Silent"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Pan Invert" FeatureId="29" NFCRecord="2" NFCOffset="18" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Tilt Invert" FeatureId="30" NFCRecord="2" NFCOffset="19" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Reset Pan/Tilt Limits" FeatureId="31" NFCRecord="3" NFCOffset="0" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Off"/>
                <Enum EnumVal="1" EnumLabel="Reset"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Enable Pan/Tilt Limits" FeatureId="32" NFCRecord="2" NFCOffset="34" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Pan Limit Min" FeatureId="33" NFCRecord="2" NFCOffset="35" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>-32767</RangeMin>
                <RangeMax>32768</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Pan Limit Max" FeatureId="34" NFCRecord="2" NFCOffset="37" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>-32767</RangeMin>
                <RangeMax>32768</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>65535</DefaultValue>
        </Feature>

        <Feature FeatureName="Tilt Limit Min" FeatureId="35" NFCRecord="2" NFCOffset="39" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>-32767</RangeMin>
                <RangeMax>32768</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Tilt Limit Max" FeatureId="36" NFCRecord="2" NFCOffset="41" FeatureType="Range">
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>-32767</RangeMin>
                <RangeMax>32768</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>65535</DefaultValue>
        </Feature>

        <Feature FeatureName="Reset IP Settings" FeatureId="37" NFCRecord="3" NFCOffset="1" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Off"/>
                <Enum EnumVal="1" EnumLabel="Reset"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="IP Address" FeatureId="38" NFCRecord="2" NFCOffset="4" FeatureType="IpAddress">
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadWrite</Access>
        </Feature>

        <Feature FeatureName="Subnet Mask" FeatureId="39" NFCRecord="2" NFCOffset="8" FeatureType="SubnetMask">
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadWrite</Access>
        </Feature>

        <Feature FeatureName="Factory Defaults" FeatureId="41" NFCRecord="3" NFCOffset="3" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Off"/>
                <Enum EnumVal="1" EnumLabel="Load"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Device Hours Total" FeatureId="42" NFCRecord="4" NFCOffset="0" FeatureType="Range">
            <Unit>hrs</Unit>
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadOnly</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
        </Feature>

        <Feature FeatureName="Device Hours Resettable" FeatureId="43" NFCRecord="2" NFCOffset="50" FeatureType="Range">
            <Unit>hrs</Unit>
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Power Cycles Total" FeatureId="44" NFCRecord="4" NFCOffset="4" FeatureType="Range">
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadOnly</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
        </Feature>

        <Feature FeatureName="Power Cycles Resettable" FeatureId="45" NFCRecord="2" NFCOffset="54" FeatureType="Range">
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="RDM UID" FeatureId="46" FeatureType="Label"> <!-- P3 ONLY -->
            <EncodeBytes>32</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="RDM UID" NFCRecord="1" NFCOffset="8" FeatureType="HEX48"> <!-- NFC ONLY -->
            <EncodeBytes>6</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="SelfTest" FeatureId="47" NFCRecord="2" NFCOffset="114" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Off"/>
                <Enum EnumVal="2" EnumLabel="Test All"/>
                <Enum EnumVal="4" EnumLabel="Test Pan/Tilt"/>
                <Enum EnumVal="6" EnumLabel="Test Effects"/>
                <Enum EnumVal="8" EnumLabel="Test LEDs"/>
                <Enum EnumVal="9" EnumLabel="Identify"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Fan Clean" FeatureId="54" NFCRecord="2" NFCOffset="111" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Disable"/>
                <Enum EnumVal="1" EnumLabel="Enable"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Lamp Hours Total" FeatureId="56" NFCRecord="4" NFCOffset="8" FeatureType="Range">
            <Unit>hrs</Unit>
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadOnly</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
        </Feature>

        <Feature FeatureName="Lamp Hours Resettable" FeatureId="57" NFCRecord="2" NFCOffset="58" FeatureType="Range">
            <Unit>hrs</Unit>
            <EncodeBytes>4</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>4294967295</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>4294967295</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Framing Mode" FeatureId="58" NFCRecord="2" NFCOffset="115" FeatureType="Discrete">
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Standard"/>
                <Enum EnumVal="1" EnumLabel="Legacy"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Reset Fixture" NFCRecord="3" NFCOffset="2" FeatureType="Discrete"> <!-- NFC ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Idle"/>
                <Enum EnumVal="1" EnumLabel="Warm Reset"/>
                <Enum EnumVal="255" EnumLabel="Cold Reset"/>
            </EnumMap>
            <DefaultValue>0</DefaultValue>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="MAC Address" NFCRecord="1" NFCOffset="2" FeatureType="HEX48"> <!-- NFC ONLY -->
            <EncodeBytes>6</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="RDM Device Model ID" NFCRecord="1" NFCOffset="0" FeatureType="HEX16"> <!-- NFC ONLY -->
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadOnly</Access>
        </Feature>

        <Feature FeatureName="SHoW ID" NFCRecord="2" NFCOffset="62" FeatureType="Range"> <!-- NFC ONLY -->
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>65535</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>65535</EncodeMax>
            </Range>
            <DefaultValue>24100</DefaultValue>
        </Feature>

        <Feature FeatureName="SHoW Key" NFCRecord="2" NFCOffset="64" FeatureType="Range"> <!-- NFC ONLY -->
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadWrite</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>500</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>500</EncodeMax>
            </Range>
            <DefaultValue>0</DefaultValue>
        </Feature>

        <Feature FeatureName="Output Power" NFCRecord="2" NFCOffset="66" FeatureType="Discrete"> <!-- NFC ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Low"/>
                <Enum EnumVal="1" EnumLabel="Mid"/>
                <Enum EnumVal="2" EnumLabel="High"/>
                <Enum EnumVal="3" EnumLabel="Max"/>
            </EnumMap>
            <DefaultValue>2</DefaultValue>
        </Feature>

        <Feature FeatureName="Antenna Type" NFCRecord="2" NFCOffset="67" FeatureType="Discrete"> <!-- NFC ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadWrite</Access>
            <EnumMap>
                <Enum EnumVal="1" EnumLabel="Omni"/>
                <Enum EnumVal="2" EnumLabel="Panel"/>
                <Enum EnumVal="3" EnumLabel="Yagi"/>
            </EnumMap>
            <DefaultValue>1</DefaultValue>
        </Feature>

        <Feature FeatureName="RSSI" NFCRecord="4" NFCOffset="12" FeatureType="Range"> <!-- NFC ONLY -->
            <Unit>dBm</Unit>
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadOnly</Access>
            <Range>
                <RangeMin>-30</RangeMin>
                <RangeMax>-120</RangeMax>
                <EncodeMin>-30</EncodeMin>
                <EncodeMax>-120</EncodeMax>
            </Range>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="RX Quality" NFCRecord="4" NFCOffset="14" FeatureType="Range"> <!-- NFC ONLY -->
            <Unit>%</Unit>
            <EncodeBytes>2</EncodeBytes>
            <Access>ReadOnly</Access>
            <Range>
                <RangeMin>0</RangeMin>
                <RangeMax>100</RangeMax>
                <EncodeMin>0</EncodeMin>
                <EncodeMax>100</EncodeMax>
            </Range>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Connection State" NFCRecord="4" NFCOffset="16" FeatureType="Discrete"> <!-- NFC ONLY -->
            <EncodeBytes>1</EncodeBytes>
            <Access>ReadOnly</Access>
            <EnumMap>
                <Enum EnumVal="0" EnumLabel="Search"/>
                <Enum EnumVal="1" EnumLabel="Locked"/>
                <Enum EnumVal="2" EnumLabel="Bound"/>
                <Enum EnumVal="3" EnumLabel="Locked and Bound"/>
            </EnumMap>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Module Manufacturer" NFCRecord="4" NFCOffset="37" FeatureType="Label"> <!-- NFC ONLY -->
            <EncodeBytes>20</EncodeBytes>
            <Access>ReadOnly</Access>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Module Model" NFCRecord="4" NFCOffset="17" FeatureType="Label"> <!-- NFC ONLY -->
            <EncodeBytes>20</EncodeBytes>
            <Access>ReadOnly</Access>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Module Firmware" NFCRecord="4" NFCOffset="57" FeatureType="Label"> <!-- NFC ONLY -->
            <EncodeBytes>20</EncodeBytes>
            <Access>ReadOnly</Access>
            <PoweredOnly>Yes</PoweredOnly>
        </Feature>

        <Feature FeatureName="Label" NFCRecord="2" NFCOffset="76" FeatureType="Label"> <!-- NFC ONLY -->
            <EncodeBytes>32</EncodeBytes>
            <Access>ReadWrite</Access>
            <DefaultValue></DefaultValue>
        </Feature>
    </ConfigurationOptions>

    <ErrorWarningMessageDefinition NFCRecord="1" NFCOffset="58" EncodeBytes="40" Access="ReadOnly">
        <EnumMap>
            <Enum EnumVal="32776" Type="WARNING" EnumShortCode="BANK" EnumLabel="BANK NO ACCESS"         />
            <Enum EnumVal="32783" Type="WARNING" EnumShortCode="BATM" EnumLabel="BATTERY MODE"           />
            <Enum EnumVal="32800" Type="WARNING" EnumShortCode="G21M" EnumLabel="GOBO 2-1 MISSING"       />
            <Enum EnumVal="32801" Type="WARNING" EnumShortCode="G22M" EnumLabel="GOBO 2-2 MISSING"       />
            <Enum EnumVal="32802" Type="WARNING" EnumShortCode="G23M" EnumLabel="GOBO 2-3 MISSING"       />
            <Enum EnumVal="32803" Type="WARNING" EnumShortCode="G24M" EnumLabel="GOBO 2-4 MISSING"       />
            <Enum EnumVal="32804" Type="WARNING" EnumShortCode="G25M" EnumLabel="GOBO 2-5 MISSING"       />
            <Enum EnumVal="32805" Type="WARNING" EnumShortCode="G26M" EnumLabel="GOBO 2-6 MISSING"       />
            <Enum EnumVal="32806" Type="WARNING" EnumShortCode="G27M" EnumLabel="GOBO 2-7 MISSING"       />
            <Enum EnumVal="33028" Type="WARNING" EnumShortCode="CMTW" EnumLabel="CMY TEMP HIGH"          />
            <Enum EnumVal="33029" Type="WARNING" EnumShortCode="EFTW" EnumLabel="EFF TEMP HIGH"          />
            <Enum EnumVal="33030" Type="WARNING" EnumShortCode="ZFTW" EnumLabel="ZF TEMP HIGH"           />
            <Enum EnumVal="33032" Type="WARNING" EnumShortCode="UITW" EnumLabel="UI TEMP HIGH"           />
            <Enum EnumVal="33033" Type="WARNING" EnumShortCode="PUTW" EnumLabel="PSU TEMP HIGH"          />
            <Enum EnumVal="33035" Type="WARNING" EnumShortCode="FTNA" EnumLabel="FROST ADJUST"           />
            <Enum EnumVal="33038" Type="WARNING" EnumShortCode="SERV" EnumLabel="SERVICE MODE"           />
            <Enum EnumVal="33043" Type="WARNING" EnumShortCode="LDTW" EnumLabel="LED DRV TMP HIGH"       />
            <Enum EnumVal="33044" Type="WARNING" EnumShortCode="BETW" EnumLabel="BEAM TMP HIGH"          />
            <Enum EnumVal="33053" Type="WARNING" EnumShortCode="FRTW" EnumLabel="FRAMING TMP HIGH"       />
            <Enum EnumVal="33056" Type="WARNING" EnumShortCode="PNTW" EnumLabel="PAN TEMP HIGH"          />
            <Enum EnumVal="33057" Type="WARNING" EnumShortCode="TLTW" EnumLabel="TILT TEMP HIGH"         />
            <Enum EnumVal="33059" Type="WARNING" EnumShortCode="F2TW" EnumLabel="FRAMING2 TMP HIGH"      />
            <Enum EnumVal="33060" Type="WARNING" EnumShortCode="LETW" EnumLabel="LED BOARD TEMP HIGH"    />
            <Enum EnumVal="33067" Type="WARNING" EnumShortCode="SRNM" EnumLabel="SR NO MISMATCH"         />
            <Enum EnumVal="33068" Type="WARNING" EnumShortCode="NOUP" EnumLabel="NO FW UPLOAD TO NODES"  />
            <Enum EnumVal="33069" Type="WARNING" EnumShortCode="FOUP" EnumLabel="FORCE UPLOAD TO NODES"  />
            <Enum EnumVal="33071" Type="WARNING" EnumShortCode="NFCW" EnumLabel="NFC WARNING"            />
            
            <Enum EnumVal="36878" Type="ERROR"   EnumShortCode="FBEP" EnumLabel="PAN FBACK ERR"          />
            <Enum EnumVal="36879" Type="ERROR"   EnumShortCode="FBET" EnumLabel="TILT FBACK ERR"         />
            <Enum EnumVal="36880" Type="ERROR"   EnumShortCode="PAER" EnumLabel="PAN ERROR"              />
            <Enum EnumVal="36881" Type="ERROR"   EnumShortCode="TIER" EnumLabel="TILT ERROR"             />
            <Enum EnumVal="36882" Type="ERROR"   EnumShortCode="PSER" EnumLabel="PAN SENSOR ERR"         />
            <Enum EnumVal="36883" Type="ERROR"   EnumShortCode="TSER" EnumLabel="TILT SENSOR ERR"        />
            <Enum EnumVal="36884" Type="ERROR"   EnumShortCode="PTCM" EnumLabel="PT SENSOR ADJUST"       />
            <Enum EnumVal="36885" Type="ERROR"   EnumShortCode="C1ER" EnumLabel="COLORWHEEL 1 ERR"       />
            <Enum EnumVal="36887" Type="ERROR"   EnumShortCode="G1ER" EnumLabel="GOBO W 1 ERR"           />
            <Enum EnumVal="36889" Type="ERROR"   EnumShortCode="G2ER" EnumLabel="GOBO W 2 ERR"           />
            <Enum EnumVal="36890" Type="ERROR"   EnumShortCode="R2ER" EnumLabel="GOBO W 2 ROT ERR"       />
            <Enum EnumVal="36891" Type="ERROR"   EnumShortCode="APER" EnumLabel="AW POS ERROR"           />
            <Enum EnumVal="36892" Type="ERROR"   EnumShortCode="ARER" EnumLabel="AW ROT ERROR"           />
            <Enum EnumVal="36893" Type="ERROR"   EnumShortCode="FOER" EnumLabel="FOCUS ERROR"            />
            <Enum EnumVal="36894" Type="ERROR"   EnumShortCode="ZOER" EnumLabel="ZOOM ERROR"             />
            <Enum EnumVal="36898" Type="ERROR"   EnumShortCode="CYER" EnumLabel="CYAN ERROR"             />
            <Enum EnumVal="36899" Type="ERROR"   EnumShortCode="MAER" EnumLabel="MAGENTA ERROR"          />
            <Enum EnumVal="36900" Type="ERROR"   EnumShortCode="YEER" EnumLabel="YELLOW ERROR"           />
            <Enum EnumVal="36901" Type="ERROR"   EnumShortCode="CTER" EnumLabel="CTC ERROR"              />
            <Enum EnumVal="36906" Type="ERROR"   EnumShortCode="IRER" EnumLabel="IRIS ERROR"             />
            <Enum EnumVal="36932" Type="ERROR"   EnumShortCode="CEPT" EnumLabel="COM ERR P/T"            />
            <Enum EnumVal="36933" Type="ERROR"   EnumShortCode="CECM" EnumLabel="COM ERR CMY"            />
            <Enum EnumVal="36934" Type="ERROR"   EnumShortCode="CEEF" EnumLabel="COM ERR EFFECT"         />
            <Enum EnumVal="36936" Type="ERROR"   EnumShortCode="CEZF" EnumLabel="COM ERR Z/F"            />
            <Enum EnumVal="36946" Type="ERROR"   EnumShortCode="COLD" EnumLabel="FIXTURE COLD"           />
            <Enum EnumVal="36983" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 1 ERR"         />
            <Enum EnumVal="36984" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 2 ERR"         />
            <Enum EnumVal="36985" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 3 ERR"         />
            <Enum EnumVal="36986" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 4 ERR"         />
            <Enum EnumVal="36987" Type="ERROR"   EnumShortCode="FAN " EnumLabel="BASE FAN 1 ERR"         />
            <Enum EnumVal="36988" Type="ERROR"   EnumShortCode="FAN " EnumLabel="BASE FAN 2 ERR"         />
            <Enum EnumVal="36989" Type="ERROR"   EnumShortCode="FAN " EnumLabel="BASE FAN 3 ERR"         />
            <Enum EnumVal="36990" Type="ERROR"   EnumShortCode="FAN " EnumLabel="BASE FAN 4 ERR"         />
            <Enum EnumVal="36993" Type="ERROR"   EnumShortCode="CMTE" EnumLabel="CMY TEMP SEN ERR"       />
            <Enum EnumVal="36994" Type="ERROR"   EnumShortCode="EFTE" EnumLabel="EFF TEMP SEN ERR"       />
            <Enum EnumVal="36995" Type="ERROR"   EnumShortCode="ZFTE" EnumLabel="ZF TEMP SEN ERR"        />
            <Enum EnumVal="36996" Type="ERROR"   EnumShortCode="PTTE" EnumLabel="PT TEMP SEN ERR"        />
            <Enum EnumVal="36997" Type="ERROR"   EnumShortCode="UITE" EnumLabel="UI TEMP SEN ERR"        />
            <Enum EnumVal="36998" Type="ERROR"   EnumShortCode="PUTE" EnumLabel="PSU TEMP SEN ERR"       />
            <Enum EnumVal="37000" Type="ERROR"   EnumShortCode="CMTC" EnumLabel="CMY TEMP CUT OFF"       />
            <Enum EnumVal="37001" Type="ERROR"   EnumShortCode="EFTC" EnumLabel="EFF TEMP CUT OFF"       />
            <Enum EnumVal="37002" Type="ERROR"   EnumShortCode="ZFTC" EnumLabel="ZF TEMP CUT OFF"        />
            <Enum EnumVal="37003" Type="ERROR"   EnumShortCode="PTTC" EnumLabel="PT TEMP CUT OFF"        />
            <Enum EnumVal="37004" Type="ERROR"   EnumShortCode="UITC" EnumLabel="UI TEMP CUT OFF"        />
            <Enum EnumVal="37005" Type="ERROR"   EnumShortCode="PUTC" EnumLabel="PSU TEMP CUT OFF"       />
            <Enum EnumVal="37007" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING1 INS ERR"       />
            <Enum EnumVal="37008" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING1 ANG ERR"       />
            <Enum EnumVal="37009" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING2 INS ERR"       />
            <Enum EnumVal="37010" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING2 ANG ERR"       />
            <Enum EnumVal="37011" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING3 INS ERR"       />
            <Enum EnumVal="37012" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING3 ANG ERR"       />
            <Enum EnumVal="37013" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING4 INS ERR"       />
            <Enum EnumVal="37014" Type="ERROR"   EnumShortCode="FSER" EnumLabel="FRAMING4 ANG ERR"       />
            <Enum EnumVal="37036" Type="ERROR"   EnumShortCode="WEER" EnumLabel="WASH EFFECT ERROR"      />
            <Enum EnumVal="37041" Type="ERROR"   EnumShortCode="CELD" EnumLabel="COM ERR LED DRV"        />
            <Enum EnumVal="37043" Type="ERROR"   EnumShortCode="LDTE" EnumLabel="LED TEMP SEN ERR"       />
            <Enum EnumVal="37049" Type="ERROR"   EnumShortCode="LDTC" EnumLabel="LED TEMP CUT OFF"       />
            <Enum EnumVal="37055" Type="ERROR"   EnumShortCode="FBEZ" EnumLabel="ZOOM FBACK ERR"         />
            <Enum EnumVal="37056" Type="ERROR"   EnumShortCode="ZSER" EnumLabel="ZOOM SENSOR ERR"        />
            <Enum EnumVal="37060" Type="ERROR"   EnumShortCode="MMER" EnumLabel="MISSING MODULE"         />
            <Enum EnumVal="37061" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 5 ERR"         />
            <Enum EnumVal="37062" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 6 ERR"         />
            <Enum EnumVal="37063" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 7 ERR"         />
            <Enum EnumVal="37064" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 8 ERR"         />
            <Enum EnumVal="37065" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 9 ERR"         />
            <Enum EnumVal="37066" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 10 ERR"        />
            <Enum EnumVal="37067" Type="ERROR"   EnumShortCode="FRTC" EnumLabel="FR TEMP CUT OFF"        />
            <Enum EnumVal="37068" Type="ERROR"   EnumShortCode="FRTE" EnumLabel="FR TEMP SEN ERR"        />
            <Enum EnumVal="37072" Type="ERROR"   EnumShortCode="FAN " EnumLabel="HEAD FAN 11 ERR"        />
            <Enum EnumVal="37079" Type="ERROR"   EnumShortCode="SEER" EnumLabel="ARTNET SOURCES EXCEED"  />
            <Enum EnumVal="37080" Type="ERROR"   EnumShortCode="SEER" EnumLabel="SACN SOURCES EXCEEDED"  />
            <Enum EnumVal="37106" Type="ERROR"   EnumShortCode="PRIE" EnumLabel="PRISM INS ERR"          />
            <Enum EnumVal="37107" Type="ERROR"   EnumShortCode="PRRO" EnumLabel="PRISM ROT ERR"          />
            <Enum EnumVal="37121" Type="ERROR"   EnumShortCode="F2TC" EnumLabel="FR2 TMP CUT OFF"        />
            <Enum EnumVal="37122" Type="ERROR"   EnumShortCode="F2TE" EnumLabel="FR2 TMP SEN ERR"        />
            <Enum EnumVal="37123" Type="ERROR"   EnumShortCode="LETC" EnumLabel="LED BOARD TMP CUT OFF"  />
            <Enum EnumVal="37124" Type="ERROR"   EnumShortCode="LETE" EnumLabel="LED BOARD SEN ERR"      />
            <Enum EnumVal="37125" Type="ERROR"   EnumShortCode="FRCE" EnumLabel="FRAMING COM ERROR"      />
            <Enum EnumVal="37126" Type="ERROR"   EnumShortCode="LFER" EnumLabel="LIGHT FROST ERROR"      />
            <Enum EnumVal="37127" Type="ERROR"   EnumShortCode="HFER" EnumLabel="HEAVY FROST ERROR"      />
            <Enum EnumVal="37128" Type="ERROR"   EnumShortCode="NFCE" EnumLabel="NFC ERROR"              />
            <Enum EnumVal="37129" Type="ERROR"   EnumShortCode="SEER" EnumLabel="ETH SOURCES EXCEEDED"   />
        </EnumMap>
    </ErrorWarningMessageDefinition>

    <SensorDefinition NFCRecord="4" Access="ReadOnly">
        <Sensor NFCOffset= "77" SensorName="UI Temperature"             SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="70.0"/>
        <Sensor NFCOffset= "83" SensorName="PSU Temperature"            SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="85.0"/>
        <Sensor NFCOffset= "89" SensorName="Pan/Tilt Temperature"       SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>
        <Sensor NFCOffset= "95" SensorName="LED Driver Temperature"     SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="80.0"/>
        <Sensor NFCOffset="101" SensorName="Light Engine Temperature 1" SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-28.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="85.0"/>
        <Sensor NFCOffset="107" SensorName="Light Engine Temperature 2" SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-28.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="85.0"/>
        <Sensor NFCOffset="113" SensorName="CMY Temperature"            SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>
        <Sensor NFCOffset="119" SensorName="Effect Temperature"         SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>
        <Sensor NFCOffset="125" SensorName="Framing Temperature 1"      SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>
        <Sensor NFCOffset="131" SensorName="Framing Temperature 2"      SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>
        <Sensor NFCOffset="137" SensorName="Zoom/Focus Temperature"     SensorType="Temperatures" SensorUnit="Centigrade" SensorPrefix="None" SensorRangeMin="-40.0" SensorRangeMax="120.0" SensorNormalMin="-20" SensorNormalMax="90.0"/>

        <Sensor NFCOffset="227" SensorName="Base Fan 1"                 SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="233" SensorName="Base Fan 2"                 SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="239" SensorName="LED Driver Fan 1"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="245" SensorName="LED Driver Fan 2"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="251" SensorName="LED Driver Fan 3"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="257" SensorName="LED Driver Fan 4"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="263" SensorName="LED Driver Fan 5"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="269" SensorName="LED Driver Fan 6"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="275" SensorName="LED Driver Fan 7"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="281" SensorName="Effect Fan 1"               SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="287" SensorName="Framing Fan 1"              SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="293" SensorName="Zoom/Focus Fan 1"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
        <Sensor NFCOffset="299" SensorName="Zoom/Focus Fan 2"           SensorType="Fans" SensorUnit="RPM" SensorPrefix="None" SensorRangeMin="0" SensorRangeMax="8400" SensorNormalMin="0" SensorNormalMax="7000"/>
    </SensorDefinition>

    <ActionDefinition>
        <ActionCategory Name="Factory Defaults">
            <Action Name="Set Factory Defaults" FeatureName="Factory Defaults" Value="1"/>
        </ActionCategory>
        <ActionCategory Name="Reset Fixture">
            <Action Name="Warm Reset" FeatureName="Reset Fixture" Value="1"/>
            <Action Name="Cold Reset" FeatureName="Reset Fixture" Value="255"/>
        </ActionCategory>
        <ActionCategory Name="Hibernation">
            <Action Name="Disable" FeatureName="Hibernation" Value="0"/>
            <Action Name="Enable" FeatureName="Hibernation" Value="1"/>
        </ActionCategory>
        <ActionCategory Name="IP Settings">
            <Action Name="Reset IP Settings" FeatureName="Reset IP Settings" Value="1"/>
        </ActionCategory>
        <ActionCategory Name="Pan/Tilt Limits">
            <Action Name="Reset Pan/Tilt Limits" FeatureName="Reset Pan/Tilt Limits" Value="1"/>
        </ActionCategory>
        <ActionCategory Name="Fan Clean">
            <Action Name="Stop" FeatureName="Fan Clean" Value="0"/>
            <Action Name="Start" FeatureName="Fan Clean" Value="1"/>
        </ActionCategory>
        <ActionCategory Name="SelfTest">
            <Action Name="Stop" FeatureName="SelfTest" Value="0"/>
            <Action Name="Test All" FeatureName="SelfTest" Value="2"/>
            <Action Name="Test Pan/Tilt" FeatureName="SelfTest" Value="4"/>
            <Action Name="Test Effects" FeatureName="SelfTest" Value="6"/>
            <Action Name="Test LEDs" FeatureName="SelfTest" Value="8"/>
            <Action Name="Identify" FeatureName="SelfTest" Value="9"/>
        </ActionCategory>
        <ActionCategory Name="Reset Counters">
            <Action Name="Reset Device Hours" FeatureName="Device Hours Resettable" Value="0"/>
            <Action Name="Reset Power Cycles" FeatureName="Power Cycles Resettable" Value="0"/>
            <Action Name="Reset Lamp Hours" FeatureName="Lamp Hours Resettable" Value="0"/>
            <Action Name="Reset All Counters">
                <Feature Name="Device Hours Resettable" Value="0"/>
                <Feature Name="Power Cycles Resettable" Value="0"/>
                <Feature Name="Lamp Hours Resettable" Value="0"/>
            </Action>
        </ActionCategory>
    </ActionDefinition>

    <UserNotes>
        None
    </UserNotes>

    <KnownIssues>
        None
    </KnownIssues>

    <RevisionHistory>
        <Revision RevisionNum="1" Date="05 Dec 2025" Author="WVE">Initial Public Release</Revision>
        <Revision RevisionNum="2" Date="12 Dec 2025" Author="WVE">Updated NDEF Record 2 Offsets</Revision>
        <Revision RevisionNum="3" Date="28 Feb 2026" Author="WVE">Added ArtNetOEMCode</Revision>
        <Revision RevisionNum="4" Date="01 Mar 2026" Author="WVE">Added Compact DMX Mode</Revision>
        <Revision RevisionNum="5" Date="30 Mar 2026" Author="WVE">Added Colour Targets</Revision>
        <Revision RevisionNum="6" Date="24 May 2026" Author="WVE">Temporary Removal of Colour Targets</Revision>
    </RevisionHistory>
</P3Model>