Modero X Accessory Media Preview Programming Instructions
Applies to the following product:
     FG5968-20 MXA-MP, Modero X Accessory - Media Preview


Necessary tools:
NETLINX Studio (if upgrading via Master)

Necessary files:

SW5968_20-KIT (SW5968_20_MXA_MP_v1_1_108.zip) containing:
   - SW5968_20-KIT Programming Instructions.txt (this file)
   - FG5968_20-Readme.txt (release notes)
   - SW5968_20_MXA_MP_v1_1_108.kit


Firmware Upgrade Preparation:

1) Extract the zip file "SW5968_20_MXA_MP_v1_1_108.zip".
2) This will create "SW5968_20_MXA_MP_v1_1_108.kit" and "SW5968_20-KIT Programming Instructions.txt".


Option 1: Upgrading via NETLINX (only option)

1) Once the Modero X is booted and connected to the MXA-MP, select the appropriate method for master connection.
2) Ensure that the MXA-MP is visible to the Modero X panel (STATUS Led on MXA-MP should toggle on/off every 5 seconds).
3) Ensure the reboot device button is checked in NETLINX Studio.
4) Begin the upgrade by downloading the "SW5968_20_MXA_MP_v1_1_108.kit".
5) After the transfer, the panel and the MXA-MP will reboot and perform the firmware upgrade.  After the upgrade, the MXA-MP unit contains the 1.1.108 release.

NOTE: The MXA-MP won't be ready for use and won't show up on the online tree in Studio until *AFTER* it's STATUS Led starts blinking again.


